{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":16,"n_cols":8,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RR-BW1"]
[]
[]
[]
[]
["","","","","FHA71AVEB99 / RR71B8W1B","FHA71AVEB99 / RR71B2W1B","FHA100AVEB9 / RR100B8W1B","FHA125AVEB9 / RR125B8W1B"]
["Hladilna kapaciteta","Nom.","","kW","7.1 (2)","7.1 (2)","9.8 (2)","12.2 (2)"]
["Piping connections","Tekočina","Zun. premer","mm","9.52","10","10","10"]
["","Plin","Zun. premer","mm","15.90","15.90","15.90","15.90"]
["","priključka","OD","mm","26","26","26","26"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,325","1,325","1,840","2,255"]
["","EER","","","2.68","2.68","2.66","2.71"]
["","Direktiva o energijskih oznakah","Hlajenje","","D","D","D","D"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","(2) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m (horizontalno); nivojska razlika: 0m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m (horizontalno); nivojska razlika: 0m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m (horizontalno); nivojska razlika: 0m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m (horizontalno); nivojska razlika: 0m"]