{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":13,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZAG-MV1"]
[]
[]
[]
[]
["","","","","FHA71AVEB / RZAG71M7V1B","FHA35AVEB / FHA35AVEB / RZAG71M7V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZAG71M7V1B","FHA50AVEB / FHA50AVEB / RZAG71M7V1B","FHA71AVEB / FHA71AVEB / RZAG100M7V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / FHA35AVEB / RZAG100M7V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZAG100M7V1B","FHA50AVEB / FHA50AVEB / FHA50AVEB / RZAG100M7V1B","FHA50AVEB / FHA50AVEB / RZAG100M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","","","","","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Hlajenje prostora","SEER","","","","","","","9.44","10.2","10.5","9.04","8.62"]
["","Letna poraba energije","","kWh/a","","","","","352","327","316","368","386"]
["","Zmogljivost","Pdizajn","kW","","","","","9.50","9.50","9.50","9.50","9.50"]
["","Razred energijske učinkovitosti","","","","","","","A+++","A+++","A+++","A+++","A+++"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","","","","7.80","7.80","7.80","7.80","7.80"]
["","SCOP/A","","","","","","","4.63","4.84","4.85","4.73","4.54"]
["","Razred energijske učinkovitosti","","","","","","","A++","A++","A++","A++","A+"]
["","Letna poraba energije","","kWh/a","","","","","2,359","2,256","2,252","2,309","2,405"]
["Grelna kapaciteta","Nom.","","kW","","","","","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Opombe","","","","","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]"]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Zunanja enota","","","","","RZAG71M7V1B","RZAG71M7V1B","RZAG71M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","","6.80 (1)","6.80 (1)","6.80 (1)"]
["Grelna kapaciteta","Nom.","","kW","","7.50 (2)","7.50 (2)","7.50 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","A++","A++","A++"]
["","Zmogljivost","Pdizajn","kW","","6.80","6.80","6.80"]
["","SEER","","","","7.80","7.58","6.55"]
["","Letna poraba energije","","kWh/a","","305","314","363"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","A+","A+","A+"]
["","Zmogljivost","Pdizajn","kW","","4.70","4.70","4.70"]
["","SCOP/A","","","","4.43","4.33","4.32"]
["","Letna poraba energije","","kWh/a","","1485","1520","1523"]