{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RZASG-MV1"]
[]
[]
[]
[]
["","","","","FHA35AVEB / FHA35AVEB / RZASG71M2V1B","FHA71AVEB / RZASG71M2V1B","FHA35AVEB / FHA35AVEB / FHA35AVEB / RZASG100M7V1B","FHA50AVEB / FHA50AVEB / RZASG100M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.80 (1)","6.80 (1)"]
["Hlajenje prostora","SEER","","","7.33","5.95"]
["","Letna poraba energije","","kWh/a","325","400"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80"]
["","Razred energijske učinkovitosti","","","A++","A+"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","4.50","4.50"]
["","SCOP/A","","","4.38","3.90"]
["","Razred energijske učinkovitosti","","","A+","A"]
["","Letna poraba energije","","kWh/a","1,438","1,616"]
["Grelna kapaciteta","Nom.","","kW","7.50 (2)","7.50 (2)"]
["Opombe","","","","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Hlajenje: T2: notranja temp. 26,6° CDB, 19,4° CWB, zun. temp. 48° CDB [Btu/hr/W]","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Zunanja enota","","","","","","RZASG100M7V1B","RZASG100M7V1B"]
["Hladilna kapaciteta","Nom.","","kW","","","9.50","9.50"]
["Grelna kapaciteta","Nom.","","kW","","","10.8","10.8"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","A++","A+"]
["","Zmogljivost","Pdizajn","kW","","","9.50","9.50"]
["","SEER","","","","","7.26","5.79"]
["","Letna poraba energije","","kWh/a","","","458","574"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","A+","A"]
["","Zmogljivost","Pdizajn","kW","","","6.00","6.00"]
["","SCOP/A","","","","","4.02","3.92"]
["","Letna poraba energije","","kWh/a","","","2090","2143"]