{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RR-BV3"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RR71B8V3B","FHQ100CAVEB / RR100B8V3B"]
["Hladilna kapaciteta","Nom.","","kW","7.1 (3)","9.8 (3)"]
["Piping connections","Liquid","OD","mm","9.52","9.52"]
["","Plin","OD","mm","15.9","15.9"]
["","priključka","OD","mm","26","26"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,350","1,875"]
["","EER","","","2.63","2.61"]
["","Direktiva o energijskih oznakah","Hlajenje","","D","D"]
["Opombe","","","","(1) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(1) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)"]
["","","","","(2) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(2) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)"]
["","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 7,5m, nivojska razlika: 0m"]
["","","","","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]