{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":6,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-K"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXS35K2V1B","FHQ50CAVEB / RXS50K2V1B"]
["Hladilna kapaciteta","Nom.","","kW","3.4","5.0"]
["Grelna kapaciteta","Nom.","","kW","4","6.0"]
["Nom. učink.","EER","","","3.58","3.18"]
["","COP","","","3.96","3.35"]
["","Letna por.energ.","","kWh","475","785"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","B"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","A","C"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","B","A"]
["","Zmogljivost","Pdizajn","kW","3.40","5.00"]
["","SEER","","","4.89","5.48"]
["","Letna poraba energije","","kWh/a","243","320"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A","A"]
["","Zmogljivost","Pdizajn","kW","3.10","4.35"]
["","SCOP/A","","","3.98","3.74"]
["","Letna poraba energije","","kWh/a","1090.75","1627.83"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]