{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":12,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L8Y1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L8Y1B","FHQ100CAVEB / RZQSG100L8Y1B","FHQ125CAVEB / RZQSG125L8Y1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG125L8Y1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQSG125L8Y1B","FHQ60CAVEB / FHQ60CAVEB / RZQSG125L8Y1B","FHQ140CAVEB / RZQSG140L7Y1B"]
["Zmogljivost hlajenja","Nom.","","kW","","","9.5","12.0","","","","13.4"]
["Hlajenje prostora","SEER","","","5.1","5.1","5.61","5.61","4.8","4.8","4.8"]
["","Letna poraba energije","","kWh/a","652","652","593","749","875","875","875"]
["","Zmogljivost","Pdizajn","kW","9.5","9.5","9.5","12","12","12","12"]
["","Razred energijske učinkovitosti","","","B","B","A+","A+","B","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.6","7.6","7.6","7.6","7.6","7.6","7.6"]
["","SCOP/A","","","3.8","3.8","3.91","4.01","3.8","3.8","3.8"]
["","Razred energijske učinkovitosti","","","A","A","A","A+","A","A","A"]
["","Letna poraba energije","","kWh/a","2,800","2,800","2,722","2,654","2,800","2,800","2,800"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","","1,480","2,075","","","","2,225"]
["","EER","","","","","3.21","2.89","","","","3.01"]
["","COP","","","","","3.61","3.62","","","","3.41"]
["","Direktiva o energijskih oznakah","Hlajenje","","","","A","C"]
["","","Ogrevanje","","","","A","A"]
["Zmogljivost gretja","Nom.","","kW","","","10.8","13.5","","","","15.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]