{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":23,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-CB / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ50CBVEB / FHQ50CBVEB / RZQG71L8Y1B","FHQ100CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ35CBVEB / FHQ35CBVEB / RZQG71L8Y1B","FHQ71CBVEB / RZQG71L8Y1B","FHQ140CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ50CBVEB / FHQ50CBVEB / RZQG100L8Y1B","FHQ100CBVEB / RZQG100L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG100L8Y1B","FHQ71CBVEB / FHQ71CBVEB / RZQG125L8Y1B","FHQ125CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG125L8Y1B","FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / FHQ35CBVEB / RZQG125L8Y1B","FHQ50CBVEB / FHQ50CBVEB / FHQ50CBVEB / RZQG125L8Y1B","FHQ60CBVEB / FHQ60CBVEB / RZQG125L8Y1B","FHQ140CBVEB / RZQG140L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","","","","","6.8","","","","","9.5","","","","12.0","","","","","13.4"]
["Hlajenje prostora","SEER","","","5.10","6.95","5.10","5.10","6.86","6.11","5.10","5.10","5.10","6.11","5.10","5.10","5.10","6.01","6.01","5.10","5.10","5.10"]
["","Letna poraba energije","","kWh/a","467","343","467","467","347","545","652","652","652","545","652","652","824","699","699","824","824","824"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","6.80","6.80","6.80","9.50","9.50","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00","12.00","12.00","12.00"]
["","Razred energijske učinkovitosti","","","B","A++","B","B","A++","A++","B","B","B","A++","B","B","B","A+","A+","B","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.00","7.60","6.00","6.00","7.60","11.30","11.30","11.30","11.30","11.30","11.30","11.30","12.71","14.13","14.13","12.71","12.71","12.71"]
["","SCOP/A","","","3.80","4.32","3.80","3.80","4.32","4.61","3.80","3.80","3.80","4.61","3.80","3.80","3.80","4.23","4.23","3.80","3.80","3.80"]
["","Razred energijske učinkovitosti","","","A","A+","A","A","A+","A++","A","A","A","A++","A","A","A","A+","A+","A","A","A"]
["","Letna poraba energije","","kWh/a","2,211","2,463","2,211","2,211","2,463","3,432","4,164","4,164","4,164","3,432","4,164","4,164","4,683","4,677","4,677","4,683","4,683","4,683"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","","","","890","","","","","1,245","","","","1,790","","","","","2,025"]
["","EER","","","","","","","3.82","","","","","3.81","","","","3.35","","","","","3.31"]
["","COP","","","","","","","4.13","","","","","4.15","","","","3.89","","","","","3.63"]
["","Direktiva o energijskih oznakah","Hlajenje","","","","","","A","","","","","A","","","","A","","","","","A"]
["","","Ogrevanje","","","","","","A","","","","","A","","","","A","","","","","A"]
["Grelna kapaciteta","Nom.","","kW","","","","","7.5","","","","","10.8","","","","13.5","","","","","15.5"]
["Opombe","","","","","","","","(1) - Letna poraba energije je v skladu z direktivo 2002/31/EC za označevanje energije","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","","","","(2) - SEER in SCOP sta v skladu z EN 14825","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]