{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS25BAVMB / RXS25L2V1B","FLXS50BAVMB / RXS50L2V1B"]
["Hladilna kapaciteta","Min.","","kW","1.2","0.9"]
["","Maks.","","kW","3.0","5.3"]
["","Nom.","","kW","2.5","4.9"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","6.35","6.35"]
["","Plin","Zun. premer","mm","9.5","12.7"]
["","Izpust","OD","mm","18.0","20"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","325","860"]
["","EER","","","3.85","2.85"]
["","COP","","","3.54","3.35"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","C"]
["","","Ogrevanje","","B","C"]
["Grelna kapaciteta","Nom.","","kW","3.4","6.1"]
["","Min.","","kW","1.2","0.9"]
["","Maks.","","kW","4.5","7.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]
["","","","","(5) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(5) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","(6) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(6) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]