{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FNA50A2VEB9 / RXM50A5V1B","FNA60A2VEB9 / RXM60A5V1B"]
["Hladilna kapaciteta","Nom.","","kW","5.00","6"]
["Grelna kapaciteta","Nom.","","kW","5.80","7"]
["Nom. učink.","EER","","","3.38","2.7"]
["","COP","","","3.34","3.11"]
["","Letna por.energ.","","kWh","740","1111"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","D"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","C","D"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A+","A"]
["","Zmogljivost","Pdizajn","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Letna poraba energije","","kWh/a","303","378"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A+","A+"]
["","Zmogljivost","Pdizajn","kW","4.00","4.6"]
["","SCOP/A","","","4.09","4.16"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","3.54","3.94"]
["","Letna poraba energije","","kWh/a","1368","1547"]
["Opombe","","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(4) - Glejte ločeno risbo za električne podatke"]