{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BB"]
[]
[]
[]
[]
["","","","","","FTXA20B2V1BB","FTXA25B2V1BB","FTXA35B2V1BB","FTXA42B2V1BB","FTXA50B2V1BB"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.02","0.022","0.023","0.028","0.030"]
["","Gretje","","Nom.","kW","0.02","0.02","0.022","0.036","0.039"]
["Ohišje","Barva","","","","Črn","Črn","Črn","Črn","Črn"]
["Mere","Enota","","Višina","mm","295","295","295","295","295"]
["","","","Širina","mm","798","798","798","798","798"]
["","","","Globina","mm","189","189","189","189","189"]
["Teža","Enota","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","11","11.5","11.9","13.1","13.5"]
["","","","Srednja","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","Nizko","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Tiho delovanje","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Gretje","Visok","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","Ogrevanje","Srednja","m³/min","8.7","9","9","10.5","11.1"]
["","","Gretje","Nizko","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Tiho delovanje","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Raven zvočne moči","Hlajenje","","","dBA","57","57","60","60","60"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","39","40","41","45","46"]
["","","","Srednja","dBA","32","33","33","37","39"]
["","","","Nizko","dBA","25","25","25","29","31"]
["","","","Tiho delovanje","dBA","19","19","19","21","24"]
["","Gretje","","Visok","dBA","39","40","41","45","46"]
["","Ogrevanje","","Srednja","dBA","32","33","33","37","42"]
["","Gretje","","Nizko","dBA","25","25","25","29","33"]
["","","","Tiho delovanje","dBA","19","19","19","21","24"]
["Hladilno sredstvo","GWP","","","","675","675","675","675","675.0"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.5","9.5","9.5","12.7","12.70"]
["","Izpust","","","","18","18","18","18","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC466A58","ARC466A58","ARC466A58","ARC466A58","ARC466A58"]
["","Ožičeni daljinski krmilnik","","","","BRC073","BRC073","BRC073","BRC073","BRC073"]
["Standardni pripomočki","Installation manual","","","","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1"]
["","Zračni filter","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Remote controller mounting plate","","","","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1"]
["Napajanje","Ime","","","","V1","V1","V1","V1","V1"]
["","Faza","","","","1~","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240","220-240"]