{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Raven zvočnega tlaka","Gretje","Visok","dBA","39","40"]
["","","Srednja","dBA","34","34"]
["","","Tiho delovanje","dBA","21","21"]
["","","Nizko","dBA","28","28"]
["","Hlajenje","Srednja","dBA","33","33"]
["","","Tiho delovanje","dBA","20","20"]
["","","Nizko","dBA","25","26"]
["","","Visok","dBA","39","40"]
["Standardni pripomočki","Priročnik za namestitev","","","1","1"]
["","Priročnik za upravljanje","","","1","1"]
["","Infrardeči daljinski upravljalnik","","","1","1"]
["","Suhe baterije AAA","","","2","2"]
["","Držalo daljinskega upravljalnika","","","1","1"]
["","Priključna plošča","","","1","1"]
["","Fiksirni vijaki notranje enote","","","2","2"]
["Krmilni sistemi","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Piping connections","Tekočina","Zun. premer","mm","6.35","6.35"]
["","Plin","Zun. premer","mm","9.50","9.50"]
["","Drain","","","18","18"]
["Vhodna moč","Hlajenje","Nom.","kW","0.017","0.019"]
["","Ogrevanje","Nom.","kW","0.020","0.020"]
["Raven zvočne moči","Cooling","","dBA","55","55"]
["","Heating","","dBA","55","55"]
["Mere","Enota","Širina","mm","770","770"]
["","","Globina","mm","225","225"]
["","","Višina","mm","286","286"]
["Ohišje","Colour","","","Bela","Bela"]
["Teža","Enota","","kg","8.50","8.50"]
["Power supply","Phase","","","1~","1~"]
["","Frekvenca","","Hz","50","50"]
["","Napetost","","V","220-240","220-240"]