{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":90,"n_cols":12,"rows_kept":90,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D"]
[]
[]
[]
[]
["","","","","","FTXF20D5V1B","FTXF25D5V1B","FTXF35D5V1B","FTXF42D5V1B","FTXF50D2V1B","FTXF60D2V1B","FTXF71D2V1B"]
["Vhodna moč","Hlajenje","","Nom.","kW","","","","","0.029","","0.032"]
["","Ogrevanje","","Nom.","kW","","","","","0.032","","0.035"]
["Ohišje","Barva","","","","","","","","Bela","","Bela"]
["Dimensions","Unit","","Height","mm","","","","","295","","295"]
["","","","Width","mm","","","","","990","","990"]
["","","","Depth","mm","","","","","263","","263"]
["Teža","Enota","","","kg","","","","","13.5","","13.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","","","","16.8","","17.3"]
["","","","Srednja","m³/min","","","","","14.4","","14.8"]
["","","","Nizko","m³/min","","","","","11.9","","12.2"]
["","","","Tiho delovanje","m³/min","","","","","10.5","","10.7"]
["","","Gretje","Visok","m³/min","","","","","17.3","","17.9"]
["","","","Srednja","m³/min","","","","","14.8","","15.8"]
["","","","Nizko","m³/min","","","","","12.2","","12.8"]
["","","","Tiho delovanje","m³/min","","","","","10.7","","11.3"]
["Sound power level","Cooling","","","dBA","","","","","59","","62"]
["","Heating","","","dBA","","","","","61","","62"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","","","","43","","46"]
["","","","Srednja","dBA","","","","","39","","42"]
["","","","Nizko","dBA","","","","","34","","37"]
["","","","Tiho delovanje","dBA","","","","","31","","34"]
["","Gretje","","Visok","dBA","","","","","42","","45"]
["","","","Srednja","dBA","","","","","38","","41"]
["","","","Nizko","dBA","","","","","33","","36"]
["","","","Tiho delovanje","dBA","","","","","30","","33"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","","","","6.35","","6.35"]
["","Plin","","Zun. premer","mm","","","","","12.7","","12.7"]
["","Drain","","","","","","","","18","","18"]
["Krmilni sistemi","Infrared remote control","","","","","","","","ARC470A1","","ARC470A1"]
["","Wired remote control","","","","","","","","BRC073A1","","BRC073A1"]
["Standardni pripomočki","Suhe baterije AAA","","","","","","","","2","","2"]
["","Priročnik za namestitev","","","","","","","","1","","1"]
["","Priročnik za upravljanje","","","","","","","","1","","1"]
["","Infrardeči daljinski upravljalnik","","","","","","","","1","","1"]
["","Držalo daljinskega upravljalnika","","","","","","","","1","","1"]
["","Priključna plošča","","","","","","","","1","","1"]
["","Fiksirni vijaki notranje enote","","","","","","","","2","","2"]
["Power supply","Ime","","","","","","","","V1","","V1"]
["","Phase","","","","","","","","1~","","1~"]
["","Frekvenca","","","Hz","","","","","50","","50"]
["","Napetost","","","V","","","","","220-240","","220-240"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.023","0.023","0.029","0.040","","0.032"]
["","Gretje","","Nom.","kW","0.023","0.023","0.029","0.040","","0.035"]
["Ohišje","Barva","","","","Bela","Bela","Bela","Bela","","Bela"]
["Mere","Enota","","Višina","mm","286","286","286","286","","295"]
["","","","Širina","mm","770","770","770","770","","990"]
["","","","Globina","mm","225","225","225","225","","263"]
["Teža","Enota","","","kg","8","8","8.5","9.00","","13.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","9.8","10","11.5","12.6","","17.3"]
["","","","Srednja","m³/min","8","8","8","9","","14.8"]
["","","","Nizko","m³/min","6","6.2","6.4","6.9","","12.2"]
["","","","Tiho delovanje","m³/min","4.3","4.3","4.4","4.9","","10.7"]
["","","Gretje","Visok","m³/min","10.4","10.4","11.9","12.8","","17.9"]
["","","Ogrevanje","Srednja","m³/min","8.3","8.4","8.6","8.8","","15.8"]
["","","Gretje","Nizko","m³/min","6.2","6.4","6.5","6.7","","12.8"]
["","","","Tiho delovanje","m³/min","5.3","5.3","5.3","5.2","","11.3"]
["Raven zvočne moči","Hlajenje","","","dBA","53","54","54","59.0","","60"]
["","Gretje","","","dBA","55","55","56","59.0","","62"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","39","40","43","45.0","","45"]
["","","","Srednja","dBA","33","33","34","36.0","","41"]
["","","","Nizko","dBA","25","26","27","30.0","","36"]
["","","","Tiho delovanje","dBA","20","20","20","22.0","","33"]
["","Gretje","","Visok","dBA","39","40","40","44.0","","44"]
["","Ogrevanje","","Srednja","dBA","34","34","35","34.0","","40"]
["","Gretje","","Nizko","dBA","28","28","29","28.0","","35"]
["","","","Tiho delovanje","dBA","21","21","21","22.0","","32"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6","6","6","6","","6.35"]
["","Plin","","Zun. premer","mm","9.5","9.5","9.5","9.50","","12.7"]
["","Izpust","","","","18","18","18","18","","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","","ARC470A1"]
["","Ožičeni daljinski krmilnik","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","","BRC073A1"]
["Standardni pripomočki","Installation manual","","","","1","1","1","1","","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","","2"]
["","General safety precautions","","","","196","196","196","196"]
["","Operation manual","","","","1","1","1","1","","1"]
["","Batteries","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2","","2"]
["","Infrared remote control","","","","1","1","1","1","","1"]
["","Mounting plate","","","","1","1","1","1","","1"]
["","Remote control holder","","","","1","1","1","1","","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","","1~"]
["","Frekvenca","","","Hz","50","50","50","50","","50"]
["","Napetost","","","V","220-440","220-440","220-440","220-440","","220-240"]
["","Ime","","","","","","","","","V1"]