{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 3MXM-N"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BW / FTXJ20MV1BS / 3MXM40N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM52N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 3MXM68N2V1B"]
["Hladilna kapaciteta","Nom.","","kW","4.00","4.00","4.0","4.00","5.20","4.00","6.00"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","467","482","482","471","593","457","787"]
["","EER","","","4.28","4.15","4.15","4.25","4.38","4.38","3.81"]
["","COP","","","4.32","3.95","3.95","4.05","4.42","4.04","3.88"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A","A","A","A"]
["","","Ogrevanje","","A","A","A","A","A","A","A"]
["Zmoglj. ogrevanja","Nom.","","kW","4.60","4.60","4.60","6.80","6.80","6.50","7.80"]
["Opombe","","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27 °CDB, 19 °CWB, zunanja temperatura: 35 °CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika : 0 m. Podatki za serijo s standardno učinkovitostjo. V uporabi so tolerance Eurovent 2015."]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","","(3) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","(4) - Glejte ločeno risbo za električne podatke"]