{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ25MV1BS","FTXJ35MV1BS"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.023","0.023","0.033"]
["","Gretje","","Nom.","kW","0.031","0.033","0.042"]
["Ohišje","Barva","","","","Srebrna","Srebrna","Srebrna"]
["Mere","Enota","","Višina","mm","303","303","303"]
["","","","Širina","mm","998","998","998"]
["","","","Globina","mm","212","212","212"]
["Teža","Enota","","","kg","12","12","12"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","8.9","8.9","10.9"]
["","","","Srednja","m³/min","6.6","6.6","7.8"]
["","","","Nizko","m³/min","4.4","4.4","4.8"]
["","","","Tiho delovanje","m³/min","2.6","2.6","2.9"]
["","","Gretje","Visok","m³/min","10.2","11.0","12.4"]
["","","Ogrevanje","Srednja","m³/min","8.4","8.6","9.6"]
["","","Gretje","Nizko","m³/min","6.3","6.3","6.9"]
["","","","Tiho delovanje","m³/min","3.8","3.8","4.1"]
["Raven zvočne moči","Hlajenje","","","dBA","54","54","59"]
["","Gretje","","","dBA","56","56","59"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","38","38","45"]
["","","","Srednja","dBA","32","32","34"]
["","","","Nizko","dBA","25","25","26"]
["","","","Tiho delovanje","dBA","19","19","20"]
["","Gretje","","Visok","dBA","40","41","45"]
["","Ogrevanje","","Srednja","dBA","34","34","37"]
["","Gretje","","Nizko","dBA","28","28","29"]
["","","","Tiho delovanje","dBA","19","19","20"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.50","9.50","9.50"]
["","Izpust","","","","18","18","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC466A9","ARC466A9","ARC466A9"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","Screw cover","","","","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Fixing screw for remote controller holder","","","","2","2","2"]
["","WLAN adapter kit","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Fixing screws for mounting plate","","","","5","5","5"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Napajanje","Ime","","","","V1","V1","V1"]
["","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]