{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":14,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MW / RXJ-M"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BW / RXJ20M3V1B","FTXJ20MV1BW / RXJ20M2V1B","FTXJ20MV1BW / RXJ20M5V1B","FTXJ25MV1BW / RXJ25M5V1B","FTXJ25MV1BW / RXJ25M2V1B","FTXJ25MV1BW / RXJ25M3V1B","FTXJ35MV1BW / RXJ35M2V1B","FTXJ35MV1BW / RXJ35M5V1B","FTXJ35MV1BW / RXJ35M3V1B","FTXJ50MV1BW / RXJ50MV1B"]
["Hladilna kapaciteta","Min.","","kW","1.30","","","","","0.90"]
["","Maks.","","kW","2.80","","","","","3.30"]
["","Nom.","","kW","2.30","2.3","2.30","2.40","2.4","2.40","3.5","3.50","","4.80"]
["Nazivna učinkovitost","Annual energy consumption","","kWh","248","248","248","254","254","254","428","428","","716"]
["","EER","","","4.64","4.64","4.64","4.73","4.73","4.73","4.09","4.09","","3.35"]
["","COP","","","5.00","5.00","5.00","4.57","4.57","4.57","4.04","4.04","","3.65"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A","A","A","A","A","","A"]
["","","Ogrevanje","","A","A","A","A","A","A","A","A","","A"]
["Grelna kapaciteta","Nom.","","kW","2.50","2.5","2.5","3.2","3.2","3.20","4","4.0","","5.80"]
["","Min.","","kW","1.30","","","","","0.90"]
["","Maks.","","kW","4.30","","","","","4.70"]
["Opombe","","","","(1) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(1) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(1) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(1) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(1) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["","","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["Hladilna kapaciteta","Min.","","kW","","","","","","","","","0.90"]
["","Nom.","","kW","","","","","","","","","3.50"]
["","Maks.","","kW","","","","","","","","","4.10"]
["Grelna kapaciteta","Min.","","kW","","","","","","","","","0.90"]
["","Nom.","","kW","","","","","","","","","4.00"]
["","Maks.","","kW","","","","","","","","","5.10"]
["Nom. učink.","EER","","","","","","","","","","","4.09"]
["","COP","","","","","","","","","","","4.04"]
["","Letna por.energ.","","kWh","","","","","","","","","428"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","","","","","","","","","A"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","","","","","","","","","A"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","","","","","","","A++"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","3.50"]
["","SEER","","","","","","","","","","","7.19"]
["","Letna poraba energije","","kWh/a","","","","","","","","","170"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","","","","","","","A++"]
["","Zmogljivost","Pdizajn","kW","","","","","","","","","3.00"]
["","SCOP/A","","","","","","","","","","","4.60"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","","","","","","","","","2.61"]
["","Letna poraba energije","","kWh/a","","","","","","","","","913"]