{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M / RXP-N"]
[]
[]
[]
[]
["","","","","FTXP50M2V1B / RXP50N5V1B","FTXP60M2V1B / RXP60N5V1B","FTXP71M2V1B / RXP71N5V1B"]
["Hladilna kapaciteta","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","5.0","6.0"]
["","Maks.","","kW","6.0","7.0"]
["Grelna kapaciteta","Min.","","kW","1.7","1.7"]
["","Nom.","","kW","6.0","7.0"]
["","Maks.","","kW","7.7","8.0"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","693","912"]
["","COP","","","3.80","3.63"]
["","EER","","","3.61","3.29"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A"]
["","","Ogrevanje","","A","A"]
["Opombe","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Hladilna kapaciteta","Min.","","kW","","","2.3"]
["","Nom.","","kW","","","7.1"]
["","Maks.","","kW","","","7.3"]
["Grelna kapaciteta","Min.","","kW","","","2.3"]
["","Nom.","","kW","","","8.2"]
["","Maks.","","kW","","","9.0"]
["Nom. učink.","EER","","","","","2.64"]
["","COP","","","","","3.19"]
["","Letna por.energ.","","kWh","","","1345"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","","","D"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","","","D"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","A++"]
["","Zmogljivost","Pdizajn","kW","","","7.1"]
["","SEER","","","","","6.20"]
["","Letna poraba energije","","kWh/a","","","401"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","A+"]
["","Zmogljivost","Pdizajn","kW","","","6.20"]
["","SCOP/A","","","","","4.01"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","","","4.24"]
["","Letna poraba energije","","kWh/a","","","2166"]
["Razpon energetske učinkovitosti","","","","","","A+++ ~ D"]