{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Outdoor unit","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Hladilna kapaciteta","Min.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Maks.","","kW","","3.0"]
["Grelna kapaciteta","Min.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Maks.","","kW","","4.00"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","","326"]
["","COP","","","","4.36"]
["","EER","","","","3.83"]
["","Direktiva o energijskih oznakah","Hlajenje","","","A"]
["","","Ogrevanje","","","A"]
["Opombe","","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["","","","","","(3) - Glejte ločeno risbo za električne podatke"]
["Hladilna kapaciteta","Min.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Maks.","","kW","2.6","","4.0"]
["Grelna kapaciteta","Min.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Maks.","","kW","3.50","","4.80"]
["Nom. učink.","EER","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Letna por.energ.","","kWh","249"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","A","","A"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","A","","A"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A++","","A++"]
["","Zmogljivost","Pdizajn","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Letna poraba energije","","kWh/a","103","","186"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A++","","A++"]
["","Zmogljivost","Pdizajn","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Pdh Zmogljvost ogrevanja pri -10°","","kW","1.99","","2.33"]
["","Letna poraba energije","","kWh/a","662","","845"]
["Razpon energetske učinkovitosti","","","","A+++ ~ D","","A+++ ~ D"]