{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9"]
[]
[]
[]
[]
["","","","","","FTXP20M5V1B9","FTXP25M5V1B9","FTXP35M5V1B9"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.019","0.02","0.032"]
["","Gretje","","Nom.","kW","0.023","0.023","0.032"]
["Ohišje","Barva","","","","Bela","Bela","Bela"]
["Mere","Enota","","Višina","mm","286","286","286"]
["","","","Širina","mm","770","770","770"]
["","","","Globina","mm","225","225","225"]
["Teža","Enota","","","kg","8.5","8.5","9"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","9.5","9.7","11.5"]
["","","","Srednja","m³/min","7.4","7.7","8.3"]
["","","","Nizko","m³/min","5.6","5.8","6.3"]
["","","","Tiho delovanje","m³/min","4.2","4.2","4.5"]
["","","Gretje","Visok","m³/min","10.4","10.4","11.5"]
["","","Ogrevanje","Srednja","m³/min","8.1","8.1","9"]
["","","Gretje","Nizko","m³/min","6.2","6.4","7"]
["","","","Tiho delovanje","m³/min","5.2","5.2","5.3"]
["Raven zvočne moči","Hlajenje","","","dBA","55","55","58"]
["","Gretje","","","dBA","55","55","58"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","39","40","43"]
["","","","Srednja","dBA","33","33","34"]
["","","","Nizko","dBA","25","26","27"]
["","","","Tiho delovanje","dBA","19","19","20"]
["","Gretje","","Visok","dBA","39","40","40"]
["","Ogrevanje","","Srednja","dBA","34","34","35"]
["","Gretje","","Nizko","dBA","28","28","29"]
["","","","Tiho delovanje","dBA","21","21","21"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.5","9.5","9.5"]
["","Izpust","","","","18","18","18"]
["Krmilni sistemi","Infrared remote control","","","","ARC480A53","ARC480A53","ARC480A53"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","2","2"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]