{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":9,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9"]
[]
[]
[]
[]
["","","","","","FTXP25N5V1B9","FTXP35N5V1B9","FTXP50N5V1B9","FTXP20N5V1B9 (Archived)"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.023","0.032","0.04","0.021"]
["","Gretje","","Nom.","kW","0.023","0.032","0.04","0.023"]
["Ohišje","Barva","","","","Bela","Bela","Bela","Bela"]
["Mere","Enota","","Višina","mm","286","286","286","286"]
["","","","Širina","mm","770","770","770","770"]
["","","","Globina","mm","225","225","225","225"]
["Teža","Enota","","","kg","9","9","9","9"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","9.9","11.5","11.8","9.6"]
["","","","Srednja","m³/min","7.5","8.3","9.3","7.5"]
["","","","Nizko","m³/min","5.8","6.3","7.6","5.6"]
["","","","Tiho delovanje","m³/min","4.4","4.5","6","4.4"]
["","","Gretje","Visok","m³/min","10.6","11.5","11.9","10.6"]
["","","Ogrevanje","Srednja","m³/min","8.6","9","9.5","8.6"]
["","","Gretje","Nizko","m³/min","6.6","7","8.2","6.6"]
["","","","Tiho delovanje","m³/min","5","5.1","7.4","5"]
["Raven zvočne moči","Hlajenje","","","dBA","55","58","59","55"]
["","Gretje","","","dBA","55","58","61","55"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","40","43","46","39"]
["","","","Srednja","dBA","33","34","39","33"]
["","","","Nizko","dBA","26","27","34","25"]
["","","","Tiho delovanje","dBA","19","20","27","19"]
["","Gretje","","Visok","dBA","40","40","44","39"]
["","Ogrevanje","","Srednja","dBA","34","35","38","34"]
["","Gretje","","Nizko","dBA","28","29","33","28"]
["","","","Tiho delovanje","dBA","21","21","30","21"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.52","9.52","12.7","9.52"]
["","Izpust","","","","18","18","18","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC480A78","ARC480A78","ARC480A78","ARC480A78"]
["","Ožičeni daljinski krmilnik","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pripomočki","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","General safety precautions","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; ekvivalentna dolžina cevi: 5m, nivojska razlika: 0m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke"]