{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RKS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RKS60F3V1B","FTXS71GV1B / RKS71FAV1B"]
["Hladilna kapaciteta","Min.","","kW","1.7","2.3"]
["","Maks.","","kW","6.7","8.5"]
["","Nom.","","kW","6.0 (1)","7.1 (1)"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","6.35","6.35"]
["","Plin","Zun. premer","mm","12.7","15.9"]
["","Izpust","OD","mm","18.0","18.0"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","995","1,175"]
["","EER","","","3.02","3.02"]
["","Direktiva o energijskih oznakah","Hlajenje","","B","D"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","(2) - Kapacitete so neto in vključujejo odbitek za hlajenje za toploto motorja notranjega ventilatorja.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["","","","","(3) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]