{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RKS-G"]
[]
[]
[]
[]
["","","","","FTXS20G2V1B / RKS20G2V1B","FTXS25G2V1B / RKS25G2V1B","FTXS35G2V1B / RKS35G2V1B","FTXS42G2V1B / RKS42G2V1B","FTXS50G2V1B / RKS50G2V1B"]
["Hladilna kapaciteta","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Maks.","","kW","2.8","3.2","4.0","5.0","5.3"]
["","Nom.","","kW","2.0 (1)","2.5 (1)","3.5 (1)","4.2 (1)","5.0 (1)"]
["Priključki napeljave","Tekočina","Zun. premer","mm","6.35","6.35","6.35","6.35","6.35"]
["","Plin","Zun. premer","mm","9.5","9.5","9.5","9.5","12.7"]
["","priključka","OD","mm","18.0","18.0","18.0","18.0","18.0"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","235","275","435","610","760"]
["","EER","","","4.26","4.55","4.02","3.44","3.29"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A","A"]
["Opombe","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]