{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":8,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60F4V1B","FTXS60GV1B / RXS60F3V1B","FTXS71GV1B / RXS71FAV1B9","FTXS71GV1B / RXS71FAV1B"]
["Hladilna kapaciteta","Min.","","kW","1.7","1.7","2.3","2.3"]
["","Maks.","","kW","6.7","6.7","8.5","8.5"]
["","Nom.","","kW","6.0 (2)","6.0 (3)","7.1 (2)","7.1 (3)"]
["Priključki cevne napeljave","Tekočina","Zun. premer","mm","6.35","6.35","6.35","6.35"]
["","Plin","Zun. premer","mm","12.7","12.7","15.9","15.9"]
["","Izpust","OD","mm","18.0","18.0","18.0","18.0"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","995","995","1,175","1,175"]
["","EER","","","3.02","3.02","3.02","3.02"]
["","COP","","","3.43","3.43","3.22","3.22"]
["","Direktiva o energijskih oznakah","Hlajenje","","B","B","B","B"]
["","","Ogrevanje","","B","B","C","C"]
["Grelna kapaciteta","Nom.","","kW","7.0 (3)","7.0 (4)","8.2 (3)","8.2 (4)"]
["","Min.","","kW","1.7","1.7","2.3","2.3"]
["","Maks.","","kW","8.0","8.0","10.2","10.2"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)"]
["","","","","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)"]
["","","","","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(4) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]