{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60L2V1B"]
["Hladilna kapaciteta","Min.","","kW","1.7"]
["","Nom.","","kW","6.0"]
["","Maks.","","kW","6.7"]
["Grelna kapaciteta","Min.","","kW","1.7"]
["","Nom.","","kW","7.0"]
["","Maks.","","kW","8.0"]
["Nom. učink.","EER","","","3.02"]
["","COP","","","3.43"]
["","Letna por.energ.","","kWh","995"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","B"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","B"]
["Priključki napeljave","priključka","OD","mm","18"]
["Priključki cevne napeljave","Plin","Zun. premer","mm","12.7"]
["","Tekočina","Zun. premer","mm","6.35"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","6.00"]
["","SEER","","","5.58"]
["","Letna poraba energije","","kWh/a","376"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","4.80"]
["","SCOP/A","","","3.89"]
["","Letna poraba energije","","kWh/a","1728"]
["Opombe","","","","(1) - 220V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]