{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","38","39","42","42","44","","46"]
["","","","Tiho delovanje","dBA","25","25","26","30","31","","34"]
["","","","Nizko","dBA","28","28","29","33","34","","37"]
["","Hlajenje","","Tiho delovanje","dBA","22","22","23","30","31","","34"]
["","","","Nizko","dBA","25","25","26","33","34","","37"]
["","","","Visok","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Hlajenje","","Nom.","dBA","32","32","34","38","39","","42"]
["Standardni pripomočki","Fotokatalizatorski filter iz titanovega apatita za čiščenje zraka","","","","2","2","2","2","2"]
["","Priročnik za upravljanje","","","","1","1","1","1","1","","1"]
["","Priročnik za namestitev","","","","1","1","1","1","1","","1"]
["","Brezžičen daljinski upravljalnik","","","","1","1","1","1","1","","1"]
["","Baterije","","","","2","2","2","2","2","","2"]
["","Držalo daljinskega upravljalnika","","","","1","1","1","1","1","","1"]
["","Fiksirni vijaki notranje enote","","","","2","2","2","2","2","","2"]
["","Priključna plošča","","","","1","1","1","1","1","","1"]
["Krmilni sist.","Infrared remote control","","","","","","","","","","ARC452A3"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Plin","","Zun. premer","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","priključka","","","","18","18","18","18","18","","18"]
["Vhodna moč","Hlajenje","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Gretje","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Raven zvočne moči","Hlajenje","","","dBA","54","54","58","58","59","","63"]
["","Gretje","","","dBA","54","55","58","58","60","","62"]
["Mere","Enota","","Širina","mm","800","800","800","800","800","","1,050"]
["","","","Globina","mm","215","215","215","215","215","","250"]
["","","","Višina","mm","295","295","295","295","295","","290"]
["Casing","Colour","","","","Bela","Bela","Bela","Bela","Bela","","Bela"]
["Teža","Enota","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frekvenca","","","Hz","50","50","50","50","50","","50"]
["","Ime","","","","V1","V1","V1","V1","V1","","V1"]
["","Napetost","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Nom.","m³/min","","","","","","16.0"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","","","","","","41"]
["Ventilator","Hitrost pretoka zraka","Gretje","Nom.","m³/min","","","","","","14.9"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","","","","","","40"]
["Vhodna moč","Hlajenje","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Gretje","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Ohišje","Barva","","","","","","","","","Bela"]
["Mere","Enota","","Višina","mm","","","","","","290"]
["","","","Širina","mm","","","","","","1050"]
["","","","Globina","mm","","","","","","250"]
["Teža","Enota","","","kg","","","","","","12"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","","","","","16.0"]
["","","","Nizko","m³/min","","","","","","11.3"]
["","","","Tiho delovanje","m³/min","","","","","","10.1"]
["","","Gretje","Visok","m³/min","","","","","","17.2"]
["","","","Nizko","m³/min","","","","","","12.6"]
["","","","Tiho delovanje","m³/min","","","","","","11.3"]
["Raven zvočne moči","Hlajenje","","","dBA","","","","","","60"]
["","Gretje","","","dBA","","","","","","59"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","","","","","45"]
["","","","Nizko","dBA","","","","","","36"]
["","","","Tiho delovanje","dBA","","","","","","33"]
["","Gretje","","Visok","dBA","","","","","","44"]
["","","","Nizko","dBA","","","","","","35"]
["","","","Tiho delovanje","dBA","","","","","","32"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","","","","","6.35"]
["","Plin","","Zun. premer","mm","","","","","","12.7"]
["","Izpust","","","","","","","","","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","","","","","","ARC452A3"]
["Standardni pripomočki","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Napajanje","Ime","","","","","","","","","V1"]
["","Faza","","","","","","","","","1~"]
["","Frekvenca","","","Hz","","","","","","50"]
["","Napetost","","","V","","","","","","220-240"]
["Standardni pripomočki","Fotokatalitski filter za čiščenje zraka s titanovim apatitom brez okvirja","","","","","","","","","","2"]
["Opombe","","","","","","","","","","","(4) - 240V"]