{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","40","","","","","","45"]
["","","","Tiho delovanje","dBA","19","","","","","","22"]
["","","","Nizko","dBA","27","","","","","","33"]
["","Hlajenje","","Tiho delovanje","dBA","19","","","","","","21"]
["","","","Nizko","dBA","24","","","","","","33"]
["","","","Visok","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Hlajenje","","Nom.","dBA","32","","","","","","39"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","","","","","","1"]
["","Priročnik za upravljanje","","","","1","","","","","","1"]
["","Brezžičen daljinski upravljalnik","","","","1","","","","","","1"]
["","Baterije","","","","2","","","","","","2"]
["","Držalo daljinskega upravljalnika","","","","1","","","","","","1"]
["","Priključna plošča","","","","1","","","","","","1"]
["","Fiksirni vijaki notranje enote","","","","2","","","","","","2"]
["","Fotokatalizatorski filter iz titanovega apatita za čiščenje zraka","","","","2","","","","","","2"]
["Krmilni sistemi","Infrard. dalj. krm.","","","","ARC466A6","","","","","","ARC466A6"]
["Piping connections","Liquid","","OD","mm","6.35","","","","","","6.35"]
["","Plin","","OD","mm","9.5","","","","","","9.5"]
["","priključka","","","","18","","","","","","18"]
["Power input","Hlajenje","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Gretje","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Raven zvočne moči","Hlajenje","","","dBA","58","","","","","","59"]
["","Gretje","","","dBA","58","","","","","","59"]
["Mere","Enota","","Width","mm","780","","","","","","900"]
["","","","Depth","mm","215","","","","","","215"]
["","","","Višina","mm","289","","","","","","298"]
["Ohišje","Barva","","","","Bela","","","","","","Bela"]
["Teža","Enota","","","kg","8","","","","","","11"]
["Power supply","Faza","","","","1~","","","","","","1~"]
["","Frekvenca","","","Hz","50","","","","","","50"]
["","Ime","","","","V1","","","","","","V1"]
["","Napetost","","","V","220-240","","","","","","220-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Ob priklopu na večsistemsko zunanjo enoto glejte specifikacije za multi zunanjo enoto, ki naj se priklopi.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Vhodna moč","Hlajenje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Gretje","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Ohišje","Barva","","","","","Bela","Bela","Bela","Bela","Bela","","Bela","Bela","Bela"]
["Mere","Enota","","Višina","mm","","215","289","215","298","215","","215","298","215"]
["","","","Širina","mm","","780","780","780","900","900","","900","900","900"]
["","","","Globina","mm","","289","215","289","215","298","","298","215","298"]
["Teža","Enota","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Srednja","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Nizko","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Tiho delovanje","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Gretje","Visok","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","Ogrevanje","Srednja","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Gretje","Nizko","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Tiho delovanje","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Raven zvočne moči","Hlajenje","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Gretje","","","dBA","","58","58","58","59","59","","59","60","60"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Srednja","dBA","","32","33","33","","37","","39","","40"]
["","","","Nizko","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Tiho delovanje","dBA","","19","19","19","19","19","","21","23","23"]
["","Gretje","","Visok","dBA","","40","41","41","45","45","","45","47","47"]
["","Ogrevanje","","Srednja","dBA","","34","34","34","","39","","39","","40"]
["","Gretje","","Nizko","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Tiho delovanje","dBA","","19","19","19","19","19","","22","24","24"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Plin","","Zun. premer","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Izpust","","","","","18","18","18","18","18","","18","18","18"]
["Krmilni sistemi","Infrard. dalj. krm.","","","","","ARC466A6","","","","","","ARC466A9"]
["Standardni pripomočki","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Napajanje","Ime","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Faza","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frekvenca","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Napetost","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilator","Hitrost pretoka zraka","Gretje","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Raven zvočnega tlaka","Gretje","","Nom.","dBA","","","34","","39","","","","40"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standardni pripomočki","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Opombe","","","","","","","","","","","(4) - 240V"]