{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BW"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.023"]
["","Gretje","","Nom.","kW","0.022"]
["Ohišje","Barva","","","","Bela"]
["Mere","Enota","","Višina","mm","295"]
["","","","Širina","mm","798"]
["","","","Globina","mm","189"]
["Teža","Enota","","","kg","12"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","13.1"]
["","","","Srednja","m³/min","9"]
["","","","Nizko","m³/min","6"]
["","","","Tiho delovanje","m³/min","4.9"]
["","","Gretje","Visok","m³/min","12.3"]
["","","Ogrevanje","Srednja","m³/min","8.2"]
["","","Gretje","Nizko","m³/min","5.8"]
["","","","Tiho delovanje","m³/min","5"]
["Raven zvočne moči","Hlajenje","","","dBA","60"]
["","Gretje","","","dBA","60"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","43"]
["","","","Srednja","dBA","32"]
["","","","Nizko","dBA","25"]
["","","","Tiho delovanje","dBA","20"]
["","Gretje","","Visok","dBA","41"]
["","Ogrevanje","","Srednja","dBA","31"]
["","Gretje","","Nizko","dBA","24"]
["","","","Tiho delovanje","dBA","19"]
["Hladilno sredstvo","GWP","","","","675"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35"]
["","Plin","","Zun. premer","mm","9.5"]
["","Izpust","","","","18"]
["Krmilni sistemi","Infrard. dalj. krm.","","","","ARC466A84"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","BRC073A4"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]