{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.029","0.053"]
["","Gretje","","Nom.","kW","0.024","0.06"]
["Ohišje","Barva","","","","Bela","Bela"]
["Mere","Enota","","Višina","mm","298","298"]
["","","","Širina","mm","804","997"]
["","","","Globina","mm","252","292"]
["Teža","Enota","","","kg","12","15"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","13.2","15.1"]
["","","","Srednja","m³/min","8.1","9.2"]
["","","","Nizko","m³/min","5.6","5.6"]
["","","","Tiho delovanje","m³/min","4.8","4.8"]
["","","Gretje","Visok","m³/min","11.7","17"]
["","","Ogrevanje","Srednja","m³/min","7.7","10"]
["","","Gretje","Nizko","m³/min","5.6","6"]
["","","","Tiho delovanje","m³/min","4.7","5.1"]
["Raven zvočne moči","Hlajenje","","","dBA","60","60"]
["","Gretje","","","dBA","59","60"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","45","46"]
["","","","Srednja","dBA","33","32"]
["","","","Nizko","dBA","25","24"]
["","","","Tiho delovanje","dBA","21","20"]
["","Gretje","","Visok","dBA","43","46"]
["","Ogrevanje","","Srednja","dBA","31","31"]
["","Gretje","","Nizko","dBA","22","22"]
["","","","Tiho delovanje","dBA","19","19"]
["Hladilno sredstvo","GWP","","","","675","675"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.5","9.5"]
["","Izpust","","","","18","18"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC466A83","ARC466A83"]
["Standardni pripomočki","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Ime","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke"]
["Standardni pripomočki","FTXTM40A2V1B","","","","","1"]