{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.032","0.037"]
["","Gretje","","Nom.","kW","0.037","0.04"]
["Ohišje","Barva","","","","Bela","Bela"]
["Mere","Enota","","Višina","mm","294","300"]
["","","","Širina","mm","811","1040"]
["","","","Globina","mm","272","295"]
["Teža","Enota","","","kg","10","14.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","11.7","15.5"]
["","","","Srednja","m³/min","8","9.2"]
["","","","Nizko","m³/min","6.3","5.7"]
["","","","Tiho delovanje","m³/min","5.2","4.6"]
["","","Gretje","Visok","m³/min","12.2","17.7"]
["","","Ogrevanje","Srednja","m³/min","7.5","11"]
["","","Gretje","Nizko","m³/min","5.1","7.5"]
["","","","Tiho delovanje","m³/min","4.1","6.3"]
["Raven zvočne moči","Hlajenje","","","dBA","60","60"]
["","Gretje","","","dBA","61","61"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","45","46"]
["","","","Srednja","dBA","33","32"]
["","","","Nizko","dBA","25","24"]
["","","","Tiho delovanje","dBA","21","20"]
["","Gretje","","Visok","dBA","45","46"]
["","Ogrevanje","","Srednja","dBA","31","31"]
["","Gretje","","Nizko","dBA","22","22"]
["","","","Tiho delovanje","dBA","19","19"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.5","9.5"]
["","Izpust","","","","16 (notranji premer priključne cevi)","16 (notranji premer priključne cevi)"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC466A55","ARC466A55"]
["","Ožičeni daljinski krmilnik","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Napajanje","Ime","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]