{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","45.0"]
["","","","Srednja","dBA","31.0"]
["","","","Tiho delovanje","dBA","19.0"]
["","","","Nizko","dBA","22.0"]
["","Hlajenje","","Medium","dBA","33.0"]
["","","","Tiho delovanje","dBA","21.0"]
["","","","Nizko","dBA","25.0"]
["","","","Visok","dBA","45.0"]
["Standardni pripomočki","Priročnik za namestitev","","","","1"]
["","Priročnik za upravljanje","","","","1"]
["","Brezžičen daljinski upravljalnik","","","","1"]
["","Suhe baterije AAA","","","","2"]
["","Držalo daljinskega upravljalnika","","","","1"]
["","Priključna plošča","","","","1"]
["","Fiksirni vijaki notranje enote","","","","2"]
["","Filter srebrnih delcev","","","","1"]
["Krmilni sistemi","Wired remote control","","","","BRC073A1"]
["","Infrard. dalj. krm.","","","","ARC466A75"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35"]
["","Plin","","Zun. premer","mm","9.50"]
["","priključka","","","","18"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.035"]
["","Gretje","","Nom.","kW","0.039"]
["Raven zvočne moči","Hlajenje","","","dBA","60.0"]
["","Gretje","","","dBA","61.0"]
["Mere","Enota","","Širina","mm","778"]
["","","","Globina","mm","272"]
["","","","Višina","mm","295"]
["Ohišje","Colour","","","","Bela"]
["Teža","Enota","","","kg","10.0"]
["Ventilator","Hitrost pretoka zraka","Ogrevanje","Visok","m³/min","12.5"]
["","","","Nizko","m³/min","4.9"]
["","","","Srednja","m³/min","7.5"]
["","","","Tiho delovanje","m³/min","4.0"]
["","","Hlajenje","Nizko","m³/min","5.3"]
["","","","Srednja","m³/min","7.8"]
["","","","Visok","m³/min","12.2"]
["","","","Tiho delovanje","m³/min","4.1"]
["Power supply","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Ime","","","","V1"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","","(3) - Glejte ločene risbe za električne podatke"]
["Vhodna moč","Hlajenje","","Nom.","kW","","0.053"]
["","Gretje","","Nom.","kW","","0.06"]
["Ohišje","Barva","","","","","Bela"]
["Mere","Enota","","Višina","mm","","299"]
["","","","Širina","mm","","998"]
["","","","Globina","mm","","292"]
["Teža","Enota","","","kg","","14.5"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","15.4"]
["","","","Srednja","m³/min","","9.5"]
["","","","Nizko","m³/min","","5.8"]
["","","","Tiho delovanje","m³/min","","4.6"]
["","","Gretje","Visok","m³/min","","17.5"]
["","","Ogrevanje","Srednja","m³/min","","10.5"]
["","","Gretje","Nizko","m³/min","","7.1"]
["","","","Tiho delovanje","m³/min","","5.9"]
["Raven zvočne moči","Hlajenje","","","dBA","","60"]
["","Gretje","","","dBA","","61"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","46"]
["","","","Srednja","dBA","","32"]
["","","","Nizko","dBA","","24"]
["","","","Tiho delovanje","dBA","","20"]
["","Gretje","","Visok","dBA","","46"]
["","Ogrevanje","","Srednja","dBA","","31"]
["","Gretje","","Nizko","dBA","","22"]
["","","","Tiho delovanje","dBA","","19"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","6.35"]
["","Plin","","Zun. premer","mm","","9.5"]
["","Izpust","","","","","18"]
["Krmilni sistemi","Infrard. dalj. krm.","","","","","ARC466A75"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","","BRC073A1"]
["Standardni pripomočki","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napajanje","Ime","","","","","V1"]
["","Faza","","","","","1~"]
["","Frekvenca","","","Hz","","50"]
["","Napetost","","","V","","220-240"]