{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-A"]
[]
[]
[]
[]
["","","","","","FTXTP25A5V1B","FTXTP35A5V1B"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.032","0.032"]
["","Gretje","","Nom.","kW","0.032","0.032"]
["Ohišje","Barva","","","","Bela","Bela"]
["Mere","Enota","","Višina","mm","286","286"]
["","","","Širina","mm","770","770"]
["","","","Globina","mm","225","225"]
["Teža","Enota","","","kg","9","9"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","11","11"]
["","","","Srednja","m³/min","7.9","7.9"]
["","","","Nizko","m³/min","5","5"]
["","","","Tiho delovanje","m³/min","3.7","3.7"]
["","","Gretje","Visok","m³/min","10.5","10.5"]
["","","Ogrevanje","Srednja","m³/min","9","9"]
["","","Gretje","Nizko","m³/min","5.5","5.5"]
["","","","Tiho delovanje","m³/min","4.4","4.4"]
["Raven zvočne moči","Hlajenje","","","dBA","58","58"]
["","Gretje","","","dBA","58","58"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","43","43"]
["","","","Srednja","dBA","35","35"]
["","","","Nizko","dBA","26","26"]
["","","","Tiho delovanje","dBA","21","21"]
["","Gretje","","Visok","dBA","43","43"]
["","Ogrevanje","","Srednja","dBA","35","35"]
["","Gretje","","Nizko","dBA","26","26"]
["","","","Tiho delovanje","dBA","21","21"]
["Hladilno sredstvo","GWP","","","","675","675"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.35","6.35"]
["","Plin","","Zun. premer","mm","9.5","9.5"]
["","Izpust","","","","18","18"]
["Krmilni sistemi","Infrared remote control","","","","ARC480A78","ARC480A78"]
["Standardni pripomočki","FTXTP25A5V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Napajanje","Ime","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","","(3) - Glejte ločeno risbo za električne podatke","(3) - Glejte ločeno risbo za električne podatke"]
["Standardni pripomočki","FTXTP35A5V1B","","","","","1"]