{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","43"]
["","","","Srednja","dBA","35"]
["","","","Tiho delovanje","dBA","21"]
["","","","Nizko","dBA","26"]
["","Hlajenje","","Srednja","dBA","35"]
["","","","Tiho delovanje","dBA","21"]
["","","","Nizko","dBA","26"]
["","","","Visok","dBA","43"]
["Standardni pripomočki","Priročnik za namestitev","","","","1"]
["","Priročnik za upravljanje","","","","1"]
["","Brezžičen daljinski upravljalnik","","","","1"]
["","Suhe baterije AAA","","","","2"]
["","Držalo daljinskega upravljalnika","","","","1"]
["","Priključna plošča","","","","1"]
["","Filter iz titanovega apatita za odstranjevanje neprijetnih vonjav","","","","2"]
["","Fiksirni vijaki notranje enote","","","","2"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Priključki napeljave","Tekočina","","Zun. premer","mm","6.35"]
["","Gas","","Zun. premer","mm","9.50"]
["","Izpust","","","","16 (notranji premer priključne cevi)"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.030"]
["","Gretje","","Nom.","kW","0.035"]
["Raven zvočne moči","Hlajenje","","","dBA","58"]
["","Gretje","","","dBA","58"]
["Mere","Enota","","Širina","mm","770"]
["","","","Globina","mm","225"]
["","","","Višina","mm","285"]
["Ohišje","Colour","","","","Bela"]
["Teža","Enota","","","kg","9.0"]
["Power supply","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Name","","","","V1"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","(1) - Glejte ločeno risbo za električne podatke"]
["Vhodna moč","Hlajenje","","Nom.","kW","","0.03"]
["","Gretje","","Nom.","kW","","0.035"]
["Ohišje","Barva","","","","","Bela"]
["Mere","Enota","","Višina","mm","","285"]
["","","","Širina","mm","","770"]
["","","","Globina","mm","","225"]
["Teža","Enota","","","kg","","9"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","","11.4"]
["","","","Srednja","m³/min","","8.2"]
["","","","Nizko","m³/min","","5.4"]
["","","","Tiho delovanje","m³/min","","4.3"]
["","","Gretje","Visok","m³/min","","10.8"]
["","","Ogrevanje","Srednja","m³/min","","7.8"]
["","","Gretje","Nizko","m³/min","","5.8"]
["","","","Tiho delovanje","m³/min","","4.9"]
["Raven zvočne moči","Hlajenje","","","dBA","","58"]
["","Gretje","","","dBA","","58"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","43"]
["","","","Srednja","dBA","","35"]
["","","","Nizko","dBA","","26"]
["","","","Tiho delovanje","dBA","","21"]
["","Gretje","","Visok","dBA","","43"]
["","Ogrevanje","","Srednja","dBA","","35"]
["","Gretje","","Nizko","dBA","","26"]
["","","","Tiho delovanje","dBA","","21"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","6.35"]
["","Plin","","Zun. premer","mm","","9.5"]
["","Izpust","","","","","16 (notranji premer priključne cevi)"]
["Krmilni sistemi","Infrared remote control","","","","","ARC480A11"]
["Krmilni sistemi","Ožičeni daljinski krmilnik","","","","","BRC944B2, BRC073A1"]
["Standardni pripomočki","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Napajanje","Ime","","","","","V1"]
["","Faza","","","","","1~"]
["","Frekvenca","","","Hz","","50"]
["","Napetost","","","V","","220-240"]