{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZA-D"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / FUA100AVEB9 / RZA200D7Y1B","FUA71AVEB9 / FUA71AVEB9 / FUA71AVEB9 / RZA200D7Y1B","FUA125AVEB9 / FUA125AVEB9 / RZA250D7Y1B (Archived)"]
["Hladilna kapaciteta","Nom.","","kW","19.0 (1)","19.0 (1)"]
["Hlajenje prostora","SEER","","","7.01","7.39"]
["","ηs,c","","%","278","292"]
["","Letna poraba energije","","kWh/a","1,625","1,543"]
["","Zmogljivost","Pdizajn","kW","19.0","19.0"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","11.2","11.2"]
["","SCOP/A","","","4.10","4.15"]
["","Letna poraba energije","","kWh/a","3,825","3,779"]
["","ηs,h","","%","161","163"]
["Grelna kapaciteta","Nom.","","kW","22.4 (2)","22.4 (2)"]
["Opombe","","","","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nominalne kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]
["Hladilna kapaciteta","Nom.","","kW","","","22.0 (1)"]
["Grelna kapaciteta","Nom.","","kW","","","24.0 (2)"]
["Hlajenje prostora","Zmogljivost","Pdizajn","kW","","","22.0"]
["","SEER","","","","","6.10"]
["","Letna poraba energije","","kWh/a","","","2163"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","","","12.1"]
["","SCOP/A","","","","","4.10"]
["","Letna poraba energije","","kWh/a","","","4132"]