{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","","","","41","46","47"]
["","","","Srednja","dBA","","","","38","42","43"]
["","","","Nizko","dBA","","","","35","39","40"]
["","Hlajenje","","Srednja","dBA","","","","38","42","43"]
["","","","Nizko","dBA","","","","35","39","40"]
["","","","Visok","dBA","","","","41","46","47"]
["Standardni pripomočki","Priročnik za upravljanje","","","","","","","1","1","1"]
["","Priročnik za namestitev","","","","","","","1","1","1"]
["","Cev izpusta","","","","","","","1","1","1"]
["","Termalna izolacijska cev","","","","","","","3","3","3"]
["","Vezice","","","","","","","10","10","10"]
["","Cevna objemka","","","","","","","1","1","1"]
["","Tesnilni material","","","","","","","4","4","4"]
["","Pritrdilna plošča podložke","","","","","","","1","1","1"]
["","Izpustni spoj","","","","","","","1","1","1"]
["","Netkano blago","","","","","","","1","1","1"]
["","Podložka","","","","","","","8","8","8"]
["","Fiksirni vijak za izpustno cev","","","","","","","5","5","5"]
["Krmilni sistemi","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Hladilna kapaciteta","Skupna kapaciteta","","Nom.","kW","","","","","","12.1"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","","","","9.52","9.52","9.52"]
["","Plin","","Zun. premer","mm","","","","15.9","15.9","15.9"]
["","priključka","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Hlajenje","","","dBA","","","","59","64","65"]
["","Gretje","","","dBA","","","","59","64"]
["Mere","Enota","","Širina","mm","","","","950","950","950"]
["","","","Globina","mm","","","","950","950","950"]
["","","","Višina","mm","","","","198","198","198"]
["Ohišje","Material","","","","","","","Smola","Smola","Smola"]
["","Barva","","","","","","","Sveže bela","Sveže bela","Sveže bela"]
["Teža","Enota","","","kg","","","","25.0","26.0","26"]
["Ventilator","Hitr. zračn. toka","Gretje","Visok","m³/min","","","","23.0","31.0","32.5"]
["","","","Srednja","m³/min","","","","19.5","25.5","26.5"]
["","","","Nizko","m³/min","","","","16.0","20.0","20.5"]
["","","Hlajenje","Nizko","m³/min","","","","16.0","20.0","20.5"]
["","","","Srednja","m³/min","","","","19.5","25.5","26.5"]
["","","","Visok","m³/min","","","","23.0","31.0","32.5"]
["Višina odvajanja","mm","","","","","","","600","600","600"]
["Grelna kapaciteta","Skupna kapaciteta","","Nom.","kW","","","","","","13.5"]
["Ohišje","Barva","","","","Sveže bela","Sveže bela","Sveže bela"]
["","Material","","","","Smola","Smola","Smola"]
["Mere","Enota","","Višina","mm","198","198","198"]
["","","","Širina","mm","950","950","950"]
["","","","Globina","mm","950","950","950"]
["Teža","Enota","","","kg","25.0","26.0","26.0"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","23.0","31.0","32.5"]
["","","","Srednja","m³/min","19.5","25.5","26.5"]
["","","","Nizko","m³/min","16.0","20.0","20.5"]
["","","Gretje","Visok","m³/min","23.0","31.0","32.5"]
["","","Ogrevanje","Srednja","m³/min","19.5","25.5","26.5"]
["","","Gretje","Nizko","m³/min","16.0","20.0","20.5"]
["Raven zvočne moči","Hlajenje","","","dBA","59","64","65"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","41","46","47"]
["","","","Srednja","dBA","38","42","43"]
["","","","Nizko","dBA","35","39","40"]
["","Gretje","","Visok","dBA","41","46","47"]
["","Ogrevanje","","Srednja","dBA","38","42","43"]
["","Gretje","","Nizko","dBA","35","39","40"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","9.52","9.52"]
["","Plin","","Zun. premer","mm","15.9","15.9","15.9"]
["","Izpust","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Višina odvajanja","mm","","","","600","600","600"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Hladilna kapaciteta","Skupna kapaciteta","","Nom.","kW","","","12.10"]
["Zmogljivost gretja","Skupna kapaciteta","","Nom.","kW","","","13.5"]