{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":11,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FUQ71CVEB / RZQG71L7V1B","FUQ71CVEB / RZQG71L7Y1B9","FUQ100CVEB / RZQG100L7V1B","FUQ100CVEB / RZQG100LY1B","FUQ100CVEB / RZQG100L7Y1B","FUQ125CVEB / RZQG125L7V1B","FUQ125CVEB / RZQG125L7Y1B"]
["Hladilna kapaciteta","Nom.","","kW","6.8","6.8","9.5","9.5","","12.0","12.0"]
["Hlajenje prostora","SEER","","","6.23","6.23","5.62","5.62","","5.03","5.03"]
["","Letna poraba energije","","kWh/a","382.022","840","591.637","591.637","","834.99","834.99"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","9.50","9.50","","12.00","12.00"]
["","Razred energijske učinkovitosti","","","A++","A++","A+","A+","","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","7.60","7.60","11.30","11.30","","14.13","14.13"]
["","SCOP/A","","","4.08","4.08","3.93","3.93","","4.44","4.44"]
["","Razred energijske učinkovitosti","","","A+","A+","A","A","","A+","A+"]
["","Letna poraba energije","","kWh/a","2,607","2,607","4,027","4,027","","4,456","4,456"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","840","840","1,230","1,230","","1,770","1,770"]
["","EER","","","4.07","4.07","4.08","4.08","","3.40","3.40"]
["","COP","","","4.47","4.47","4.04","4.04","","4.04","4.04"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A","","A","A"]
["","","Ogrevanje","","A","A","A","A","","A","A"]
["Grelna kapaciteta","Nom.","","kW","7.5","7.5","10.8","10.8","","13.5","13.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]
["Hladilna kapaciteta","Nom.","","kW","","","","","9.5"]
["Grelna kapaciteta","Nom.","","kW","","","","","10.8"]
["Nom. učink.","EER","","","","","","","4.08"]
["","COP","","","","","","","4.04"]
["","Letna por.energ.","","kWh","","","","","1230"]
["Imenska učinkovitost","Direktiva o energijskih oznakah","Hlajenje","","","","","","A"]
["Nazivna učinkovitost","Direktiva o energijskih oznakah","Ogrevanje","","","","","","A"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","","","","","A+"]
["","Zmogljivost","Pdizajn","kW","","","","","9.5"]
["","SEER","","","","","","","5.62"]
["","Letna poraba energije","","kWh/a","","","","","592"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","","","","","A"]
["","Zmogljivost","Pdizajn","kW","","","","","11.3"]
["","SCOP/A","","","","","","","3.93"]
["","Letna poraba energije","","kWh/a","","","","","4027"]