{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / AZAS-MY"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / AZAS100MUY","FVA125AMVEB / AZAS125MUY","FVA140AMVEB / AZAS140MUY"]
["Hladilna kapaciteta","Nom.","","kW","9.5","12.1 (1)","13.4 (1)"]
["Grelna kapaciteta","Nom.","","kW","10.8 (2)","13.5 (2)","15.5 (2)"]
["Hlajenje prostora","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","9.5","12.1","13.4"]
["","SEER","","","5.5","5.3","5.4"]
["","Letna poraba energije","","kWh/a","605","1370","1489"]
["Ogrevanje prostora (Povprečno podnebje)","Razred energijske učinkovitosti","","","A"]
["","Zmogljivost","Pdizajn","kW","6","6","7.8"]
["","SCOP/A","","","3.79","3.56","3.81"]
["","Letna poraba energije","","kWh/a","2217","2360","2866"]
["Opombe","","","","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m","(1) - Nom. kapacitete hlajenja temeljijo na: notranja temperatura: 27°CDB, 19°CWB, zunanja temperatura: 35°CDB, ekvivalentna napeljava hladilnega sredstva: 5 m, višinska razlika: 0 m"]
["","","","","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m.","(2) - Nominalne kapacitete gretja temeljijo na: notranji temperaturi: 20° CDB; zunanja temperatura: 7° CDB, 6° CWB, ekvivalentna dolžina cevi hladilnega sredstva: 5m, nivojska razlika: 0m."]