{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L7V1B","FVQ71CVEB / RZQG71L7Y1B9","FVQ100CVEB / RZQG100L7V1B","FVQ100CVEB / RZQG100L7Y1B","FVQ125CVEB / RZQG125L7V1B","FVQ125CVEB / RZQG125L7Y1B","FVQ140CVEB / RZQG140L7V1B"]
["Hladilna kapaciteta","Nom.","","kW","6.8","6.8","9.5","9.5","12.0","12.0","13.4"]
["Hlajenje prostora","SEER","","","5.16","5.16","5.59","5.59","4.77","4.77"]
["","Letna poraba energije","","kWh/a","461.24","461.24","594.812","594.812","880.503","880.503"]
["","Zmogljivost","Pdizajn","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Razred energijske učinkovitosti","","","A","A","A","A","B","B"]
["Ogrevanje prostora (Povprečno podnebje)","Zmogljivost","Pdizajn","kW","6.33","6.33","11.30","11.30","11.30","11.30"]
["","SCOP/A","","","3.81","3.81","3.80","3.80","3.85","3.85"]
["","Razred energijske učinkovitosti","","","A","A","A","A","A","A"]
["","Letna poraba energije","","kWh/a","2,325.984","2,325.984","4,165","4,165","4,111","4,111"]
["Nazivna učinkovitost","Letna por.energ.","","kWh","1,010","1,010","1,245","1,245","1,870","1,870","2,085"]
["","EER","","","3.37","3.37","3.81","3.81","3.21","3.21","3.21"]
["","COP","","","3.64","3.64","4.14","4.14","3.70","3.70","3.61"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A","A","A","A"]
["","","Ogrevanje","","A","A","A","A","A","A","A"]
["Grelna kapaciteta","Nom.","","kW","7.5","7.5","10.8","10.8","13.5","13.5","15.5"]
["Opombe","","","","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(2) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]