{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXLG-K"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXLG25K2V1B","FVXG25K2V1B / RXLG25K3V1B","FVXG35K2V1B / RXLG35K3V1B","FVXG35K2V1B / RXLG35K2V1B","FVXG50K2V1B / RXLG50K2V1B","FVXG50K2V1B / RXLG50K3V1B"]
["Hladilna kapaciteta","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Maks.","","kW","3.0","3.0","3.8","3.8","5.6","5.6"]
["","Nom.","","kW","2.5 (3)","2.5 (2)","3.5 (2)","3.5 (3)","5.0 (2)","5.0 (2)"]
["Priključki cevne napeljave","Liquid","Zun. premer","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gas","Zun. premer","mm","9.5","9.5","9.5","9.5","12.7","12.7"]
["","Drain","OD","mm","","18.0","18.0","","18.0","18.0"]
["Nazivna učinkovitost","Annual energy consumption","","kWh","275","275","475","476","760","760"]
["","EER","","","4.55","4.55","3.68","3.68","3.29 (1)","3.29 (1)"]
["","COP","","","4.36","4.36","3.72","3.72","3.67 (1)","3.67 (1)"]
["","Direktiva o energijskih oznakah","Hlajenje","","A","A","A","A","A","A"]
["","","Ogrevanje","","A","A","A","A","A","A"]
["Grelna kapaciteta","Nom.","","kW","3.4 (4)","3.4 (3)","4.5 (3)","4.5 (4)","5.8 (3)","5.8 (3)"]
["","Min.","","kW","1.3","1.3","1.4","1.4","1.7","1.7"]
["","Maks.","","kW","4.5","4.5","5.0","5.0","8.1","8.1"]
["Opombe","","","","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - Energijska oznaka: lestvica od A (najvišja učinkovitost) do G (najmanjša učinkovitost)","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU","(1) - EER/COP v skladu z Eurovent 2012, za uporabo samo zunaj EU"]
["","","","","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5 m (horizontalno)","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5 m (horizontalno)","(2) - Letna poraba energije: na podlagi povprečne rabe 500 obratovalnih ur na leto pri polni obremenitvi (nominalni pogoji)","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(2) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5 m (horizontalno)","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(3) - Hlajenje: Notranja temperatura 27° CDB, 19,0° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5 m (horizontalno)","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(3) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["","","","","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(4) - 220V","(4) - 220V","(4) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5 m (horizontalno)","(4) - 220V","(4) - 220V"]
["","","","","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(5) - 230V","(5) - 230V","(5) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(5) - 230V","(5) - 230V"]
["","","","","","(6) - 240V","(6) - 240V","","(6) - 240V","(6) - 240V"]
["","","","","","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem.","(7) - Nom. učink.: hlajenje pri 35°/27° nom. obrem., gretje pri 7°/20° nom. obrem."]