{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Vhodna moč","Hlajenje","","Nom.","kW","0.02","0.02","0.03"]
["","Gretje","","Nom.","kW","0.02","0.03","0.03"]
["Ohišje","Barva","","","","Bela","Bela","Bela"]
["Mere","Enota","","Višina","mm","600","600","600"]
["","","","Širina","mm","750","750","750"]
["","","","Globina","mm","238","238","238"]
["Teža","Enota","","","kg","17","17","17"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Visok","m³/min","8.7","9.2","11.6"]
["","","","Srednja","m³/min","7","7","9"]
["","","","Nizko","m³/min","4.9","4.9","6.6"]
["","","","Tiho delovanje","m³/min","4.1","4.1","5.4"]
["","","Gretje","Visok","m³/min","9.2","9.8","12.8"]
["","","Ogrevanje","Srednja","m³/min","7.2","7.2","10"]
["","","Gretje","Nizko","m³/min","5.6","5.6","8.4"]
["","","","Tiho delovanje","m³/min","4.1","4.1","5.9"]
["Raven zvočne moči","Hlajenje","","","dBA","52","53","61"]
["","Gretje","","","dBA","52","53","62"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","38","39","44"]
["","","","Srednja","dBA","32","32","38"]
["","","","Nizko","dBA","25","25","31"]
["","","","Tiho delovanje","dBA","20","20","27"]
["","Gretje","","Visok","dBA","38","39","46"]
["","Ogrevanje","","Srednja","dBA","32","32","40"]
["","Gretje","","Nizko","dBA","25","25","35"]
["","","","Tiho delovanje","dBA","19","19","29"]
["Hladilno sredstvo","GWP","","","","675","675","675"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","6.4","6.4","6.4"]
["","Plin","","Zun. premer","mm","9.5","9.5","12.7"]
["","Izpust","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Krmilni sistemi","Infrardeči daljinski upravljalnik","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Ožičeni daljinski krmilnik","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pripomočki","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Napajanje","Ime","","","","V1","V1","V1"]
["","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB; zunanja temperatura 35° CDB; 24° CWB; ekvivalentna dolžina cevi: 5m"]
["","","","","","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m","(2) - Ogrevanje: Notranja temperatura 20° CDB; zunanja temperatura 7° CDB, 6° CWB; ekvivalentna dolžina cevi hladilnega sredstva: 5m"]
["Standardni pripomočki","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]