{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWR-AT"]
[]
[]
[]
[]
["","","","","","FWR02AATV3","FWR03AATV3","FWR06AATV3","FWR08AATV3"]
["Raven zvočnega tlaka","Nizko","","","dBA","35 (6)","31 (6)","38 (6)","44 (5)"]
["","Visok","","","dBA","45 (6)","43 (6)","51 (6)","62 (5)"]
["Skupna raven zvočne moči","Nizko","","","dBA","40 (4)","36 (4)","43 (4)","49 (4)"]
["","Visoko","","","dBA","50 (4)","48 (4)","56 (4)","67 (4)"]
["Tok vode","Hlajenje","","Nizko","l/h","234 (1)","302 (1)","515 (1)","706 (1)"]
["","","","Visoko","l/h","337 (1)","503 (1)","774 (1)","1,376 (1)"]
["","Ogrevanje","","Visoko","l/h","373 (2)","506 (2)","866 (2)","1,455 (2)"]
["","","","Nizko","l/h","260 (2)","301 (2)","575 (2)","764 (2)"]
["","Padec vodnega tlaka","Ogrevanje","Visoko","kPa","12 (2)","11 (2)","14 (2)","18 (2)"]
["","","","Nizko","kPa","6 (2)","5 (2)","7 (2)","6 (2)"]
["","","Hlajenje","Visoko","kPa","12 (1)","11 (1)","14 (1)","20 (1)"]
["","","","Nizko","kPa","6 (1)","5 (1)","7 (1)","6 (1)"]
["Priključki napeljave","priključka","","OD","mm","16","16","16","16"]
["Vhodna moč","Visoko","","","kW","0.019","0.016","0.033","0.087"]
["","Nizko","","","kW","0.01","0.01","0.01","0.013"]
["Dovoljena temperatura vode","Ogrevanje","","Maks.","°C","95.000","95.000","95.000","95.000"]
["","","","Min.","°C","5.00","5.00","5.00","5.00"]
["","Hlajenje","","Min.","°C","5","5","5","5"]
["","","","Maks.","°C","95.0","95.0","95.0","95.0"]
["Mere","Enota","","Širina","mm","774","984","1,190","1,404"]
["","","","Globina","mm","246","246","246","271"]
["","","","Višina","mm","564","564","564","564"]
["Vodni priključki","Dodatna tuljava","","","palcev","","1/2\""]
["","Primarna tuljava","","","palcev","1/2\"","1/2\"","1/2\"","3/4 \""]
["Ohišje","Barva","","","","Bela - RAL9010","Bela - RAL9010","Bela - RAL9010"]
["Teža","Enota","","","kg","21.2","27.5","33.6","43.1"]
["Ventilator","Hitrost pretoka zraka","","Nizko","m³/h","211","241","470","642"]
["","","","Visok","m³/h","344","442","785","1,393"]
["Power supply","Tip","","","","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50"]
["","Faza","","","","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50"]
["","Napetost","","","V","230","230","230","230"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K."]
["","","","","","(2) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 45°C, padec temperature vode 5K."]
["","","","","","(3) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 65°C, padec temperature vode 10K.","(3) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 65°C, padec temperature vode 10K.","(3) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 65°C, padec temperature vode 10K.","(3) - Ogrevanje: notranja temp. 20°CDB, 15°CWB; vhodna temperatura vode 65°C, padec temperature vode 10K."]
["","","","","","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741"]
["","","","","","(5) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","(5) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","(5) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","(5) - Raven zvočnega tlaka je merjena z mikrofonom, postavljenim na razdalji 1 m od enote."]
["","","","","","(6) - Raven zvočnega tlaka je merjena z mikrofonom, postavljenim na razdalji 1 m od enote.","(6) - Raven zvočnega tlaka je merjena z mikrofonom, postavljenim na razdalji 1 m od enote.","(6) - Raven zvočnega tlaka je merjena z mikrofonom, postavljenim na razdalji 1 m od enote."]