{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":10,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWT-HTV"]
[]
[]
[]
[]
["","","","","","FWT02HATVMV1","FWT03HATVMV1","FWT04HATVMV1","FWT05HATVMV1","FWT06HATVMV1"]
["Zmogljivost hlajenja (standardni pogoji)","Občutna zmogljivost 2-cevi","","Nizko","kW","1.52 (1)","1.61 (1)","1.88 (1)","2.64 (1)","3.19 (1)"]
["","","","Visoko","kW","1.77 (1)","2.07 (1)","2.61 (1)","3.56 (1)","4.19 (1)"]
["","Skupna zmogljivost 2-cevi","","Nizko","kW","2.11 (1)","2.23 (1)","2.58 (1)","3.37 (1)","4.07 (1)"]
["","","","Visoko","kW","2.43 (1)","2.70 (1)","3.49 (1)","4.54 (1)","5.28 (1)"]
["Zmogljivost ogrevanja (standardni pogoji)","Zmogljivost 2-cevi","","Nizko","kW","1.96 (2)","2.02 (2)","2.64 (2)","4.04 (2)","4.54 (2)"]
["","","","Visoko","kW","2.73 (2)","2.96 (2)","3.72 (2)","4.89 (2)","6.24 (2)"]
["Vhodna moč","Nizko","","","kW","0.007","0.007","0.010","0.015","0.020"]
["","Visoko","","","kW","0.010","0.012","0.020","0.025","0.043"]
["Mere","Enota","","Višina","mm","288","288","288","317","317"]
["","","","Širina","mm","870","870","870","1089","1089"]
["","","","Globina","mm","234","234","234","275","275"]
["Teža","Enota","","","kg","10","10","10","14.6","14.6"]
["Ohišje","Barva","","","","Bela","Bela","Bela","Bela","Bela"]
["Ventilator","Hitrost pretoka zraka","","Nizko","m³/h","340 (3)","357 (3)","425 (3)","663 (3)","782 (3)"]
["","","","Visok","m³/h","442 (3)","476 (3)","629 (3)","866 (3)","1053 (3)"]
["Skupna raven zvočnega tlaka","Nizko","","","dBA","39 (4)","39 (4)","45 (4)","48 (4)","51 (4)"]
["","Visoko","","","dBA","46 (4)","49 (4)","55 (4)","55 (4)","59 (4)"]
["Raven zvočnega tlaka","Nizko","","","dBA","25 (5)","26 (5)","32 (5)","34 (5)","39 (5)"]
["","Visok","","","dBA","34 (5)","35 (5)","42 (5)","42 (5)","46 (5)"]
["Tok vode","Hlajenje","","Nizko","l/h","364","439","444","583","701"]
["","","","Visoko","l/h","419","467","599","781","906"]
["","Ogrevanje","","Nizko","l/h","364","439","444","583","701"]
["","","","Visoko","l/h","419","467","599","781","906"]
["","Padec vodnega tlaka","Hlajenje","Nizko","kPa","17","18","24","13","20"]
["","","","Visoko","kPa","26","30","46","25","33"]
["","","Ogrevanje","Nizko","kPa","18 (2)","20 (2)","23 (2)","19 (2)","28 (2)"]
["","","","Visoko","kPa","27 (2)","32 (2)","44 (2)","31 (2)","45 (2)"]
["Priključki napeljave","Voda","","Dovod","","3/4\"","3/4\"","3/4\"","3/4\"","3/4\""]
["","","","Odvod","","3/4\"","3/4\"","3/4\"","3/4\"","3/4\""]
["","priključka","","OD","mm","16.5","16.5","16.5","16.5","16.5"]
["Napajanje","Tip","","","","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50","220-240 / 1 / 50"]
["","Faza","","","","1~","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240","220-240"]
["Vhodni tok","Nizko","","","A","0.07","0.07","0.09","0.11","0.16"]
["","Visok","","","A","0.10","0.10","0.16","0.22","0.32"]
["Motor ventilatorja","Vhodna moč","","Nizka","kW","0.007","0.007","0.010","0.015","0.020"]
["","","","Visoka","kW","0.010","0.012","0.020","0.025","0.043"]
["Opombe","","","","","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K.","(1) - Hlajenje: Notranja temperatura 27° CDB, 19° CWB, vstopna temperatura vode 7° C, dvig temperature vode 5K."]
["","","","","","(2) - Ogrevanje: 2 cevi: zrak 20°CST; dovod vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: 2 cevi: zrak 20°CST; dovod vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: 2 cevi: zrak 20°CST; dovod vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: 2 cevi: zrak 20°CST; dovod vode 45°C, padec temperature vode 5K.","(2) - Ogrevanje: 2 cevi: zrak 20°CST; dovod vode 45°C, padec temperature vode 5K."]
["","","","","","(3) - Pretok zraka pri 0Pa ESP","(3) - Pretok zraka pri 0Pa ESP","(3) - Pretok zraka pri 0Pa ESP","(3) - Pretok zraka pri 0Pa ESP","(3) - Pretok zraka pri 0Pa ESP"]
["","","","","","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741","(4) - Raven zvočne moči po ISO3741"]
["","","","","","(5) - Zvočni tlak, merjen 1 m pred enoto in 0,8 m pod navpično središčnico enote (JIS C 9612).","(5) - Zvočni tlak, merjen 1 m pred enoto in 0,8 m pod navpično središčnico enote (JIS C 9612).","(5) - Zvočni tlak, merjen 1 m pred enoto in 0,8 m pod navpično središčnico enote (JIS C 9612).","(5) - Zvočni tlak, merjen 1 m pred enoto in 0,8 m pod navpično središčnico enote (JIS C 9612).","(5) - Zvočni tlak, merjen 1 m pred enoto in 0,8 m pod navpično središčnico enote (JIS C 9612)."]