{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CM3"]
[]
[]
[]
[]
["","","","","","JEHCCU0140CM3","JEHCCU0170CM3"]
["Kapac. hlajenja","Sred. temp.","R-407F","Nom.","kW","2.08"]
["Zmogljivost hlajenja","Srednja temperatura","R-449A","Nazivno","kW","2.15","2.57"]
["Kapac. hlajenja","Sred. temp.","R-407A","Nom.","kW","1.92"]
["Zmogljivost hlajenja","Srednja temperatura","R-448A","Nazivno","kW","2.15","2.57"]
["Vhodna moč","Sred. temp.","R-407F","Nom.","kW","1.12"]
["","","R-407A","Nom.","kW","1.16"]
["","Srednja temperatura","R-448A","Nazivno","kW","1.07","1.46"]
["","","R-449A","Nazivno","kW","1.07","1.46"]
["COP","Srednja temperatura","","R-448A","","2","1.76"]
["","","","R-449A","","2","1.76"]
["","Sred. temp.","","R-407F","","1.85"]
["","","","R-407A","","1.66"]
["Parametri pri polni obrem. in okoliški temp. 32°C (Točka A)","R-407A","Te -10°C","Nazivna zmogljivost hlajenja (PA)","kW","1.92"]
["","","","Nazivna vhodna moč (DA)","kW","1.16"]
["","","","Nazivni COP (COPA)","","1.66"]
["","R-407F","Te -10°C","Nazivna zmogljivost hlajenja (PA)","kW","2.08"]
["","","","Nazivna vhodna moč (DA)","kW","1.12"]
["","","","Nazivni COP (COPA)","","1.85"]
["Parametri pri polni obremenitvi in temperaturi okolice 32 °C (Točka A)","R-448A","Te -10 °C","Naz. zmoglj. hlaj. (PA)","kW","2.15","2.57"]
["","","","Nazivna vhodna moč (DA)","kW","1.07","1.46"]
["","","","Nazivni COP (COPA)","","2","1.76"]
["Parametri pri polni obrem. in temp. okolice 32 °C (Točka A)","R-449A","Te -10 °C","Naz. zmoglj. hlaj. (PA)","kW","2.15","2.57"]
["Parametri pri polni obremenitvi in temperaturi okolice 32 °C (Točka A)","R-449A","Te -10 °C","Nazivna vhodna moč (DA)","kW","1.07","1.46"]
["","","","Nazivni COP (COPA)","","2","1.76"]
["Parametri pri polni obrem. in okoliški temp. 25°C","R-407A","Te -10°C","Deklarirani COP (COP2)","","1.78"]
["","R-407F","Te -10°C","Deklarirani COP (COP2)","","2.11"]
["Parametri pri polni obremenitvi in temperaturi okolice 25 °C","R-448A","Te -10 °C","Vhodna moč (D2)","kW","1.02","1.4"]
["","","","Deklarirani COP (COP2)","","2.31","2.01"]
["","R-449A","Te -10 °C","Vhodna moč (D2)","kW","1.02","1.4"]
["","","","Deklarirani COP (COP2)","","2.31","2.01"]
["Parametri pri polni obrem. in okoliški temp. 43°C","R-407A","Te -10°C","Deklarirani COP (COP3)","","1.48"]
["","R-407F","Te -10°C","Deklarirani COP (COP3)","","1.49"]
["Parametri pri polni obremenitvi in temperaturi okolice 43 °C","R-448A","Te -10 °C","Deklarirani COP (COP3)","","1.53","1.43"]
["","R-449A","Te -10 °C","Parametri pri polni obremenitvi in temperaturi okolice 43 °C-=-R-449A-=-Te -10 °C-=-Deklarirani COP (COP3)","","1.53","1.43"]
["Ventilator","Tip","","","","Aksialen","Aksialen"]
["Mere","Enota","","Višina","mm","662","662"]
["","","","Širina","mm","1101","1101"]
["","","","Globina","mm","444","444"]
["Teža","Enota","","","kg","67","68"]
["Ohišje","Barva","","","","Svetlo siva","Svetlo siva"]
["Hladilno sredstvo","Tip 2","","","","R-407A"]
["","Tip 3","","","","R-407F"]
["","Tip 5","","","","R-448A","R-448A"]
["Hlad. sred.","GWP tip 5","","","","1387","1387"]
["","GWP tip 2","","","","2107"]
["","GWP tip 3","","","","1825"]
["Napajanje","Faza","","","","3~","3~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","400","400"]
["Opombe","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Raven zvočnega tlaka je merjena na 10 m v sobi brez odmeva","(2) - Raven zvočnega tlaka je merjena na 10 m v sobi brez odmeva"]
["","","","","","(3) - Delovanje odvisno od fluoriranih toplogrednih plinov","(3) - Delovanje odvisno od fluoriranih toplogrednih plinov"]