{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA50B2V1B","RXA50B5V1B"]
["Mere","Enota","","Višina","mm","734","734","734"]
["","","","Širina","mm","870","870","954"]
["","","","Globina","mm","373","373","401"]
["Teža","Enota","","","kg","50","50","49"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","-10","-10","-10"]
["","","","Maks.","° CDB","46","46","46"]
["","Gretje","Okolje","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","48.0","48.0","48"]
["","Gretje","","Nom.","dBA","48.0","48.0","48"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32"]
["","Polnitev","","","kg","1.10","1.10","1.1"]
["","Polnjenje","","","tCO2Eq","0.75","0.75","0.75"]
["","GWP","","","","675","675","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","30","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","20","20","20"]
["Standardni pripomočki","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240"]
["Kompresor","Tip","","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Opombe","","","","","","","(1) - Glejte ločeno risbo za obratovalno območje"]
["","","","","","","","(2) - Glejte ločeno risbo za električne podatke"]
["","","","","","","","(3) - Vsebuje fluorirane toplogredne pline"]