{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":16,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ20M2V1B","RXJ20M3V1B","RXJ20M5V1B","RXJ25M2V1B","RXJ25M3V1B","RXJ25M5V1B","RXJ35M2V1B","RXJ35M3V1B","RXJ35M5V1B","RXJ50MV1B","RXJ50M2V1B"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","29.3","","","29.3","","","29.3","","","38.5"]
["","","Ogrevanje","Izjemno nizka","m³/min","25.6","","","25.6","","","25.6","","","34.3"]
["","","","Izjemno nizka","cfm","1035","","","1035","","","1035","","","1359"]
["","","Ogrevanje","Izjemno nizka","cfm","904","","","904","","","904","","","1211"]
["Mere","Enota","","Višina","mm","550","550","550","550","550","550","550","550","550","735","735"]
["","","","Širina","mm","765","765","765","765","765","765","765","765","765","825","825"]
["","","","Globina","mm","285","285","285","285","285","285","285","285","285","300","300"]
["Teža","Enota","","","kg","34","32","32","34","32","32","34","32","32","44","44"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","760","","","760","","","760","","","620"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","740","","","740","","","740","","","620"]
["Kompresor","Type","","","","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46","46","46","46","46","46"]
["","Gretje","Okolje","Min.","° CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18","18","18","18","18","18","18","18","20"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","46","","","46","","","48","","","48","48"]
["","","","Nom.","dBA","","46","46","","46","46","","49","49"]
["","","","Nizko","dBA","","","","","","","","","","","45"]
["","Gretje","","Visok","dBA","47","","","47","","","48","","","48","48"]
["","","","Nom.","dBA","","47","47","","47","47","","49","49"]
["","","","Nizko","dBA","","","","","","","","","","","45"]
["Hladilno sredstvo","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Polnitev","","","kg","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76","1.30","1.3"]
["","Polnjenje","","","tCO2Eq","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52","0.9","0.88"]
["","GWP","","","","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0","675","675"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20","20","20","20","20","20","20","20","20","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0","20"]
["Standardni pripomočki","Installation manual","","","","1","1","","1","1","","1","1","","1"]
["","Drain plug","","","","1","1","","1","1","","1","1","","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Opombe","","","","","(1) - 220V","","","(1) - 220V","","","(1) - 220V","","","(1) - 220V"]
["","","","","","(2) - 230V","","","(2) - 230V","","","(2) - 230V","","","(2) - 230V"]
["","","","","","(3) - 240V","","","(3) - 240V","","","(3) - 240V","","","(3) - 240V"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Standardni pripomočki","Refrigerant charge label","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","1","","","1","","","1"]