{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","","","30.1","30.6","48.9"]
["","","Ogrevanje","Izjemno nizka","m³/min","","","25.6","27.2","43.1"]
["","","","Izjemno nizka","cfm","","","1063","1080","1727"]
["","","Ogrevanje","Izjemno nizka","cfm","","","904","960","1522"]
["Mere","Enota","","Višina","mm","550","550","550","550","735"]
["","","","Širina","mm","765","765","765","765","825"]
["","","","Globina","mm","285","285","285","285","300"]
["Teža","Enota","","","kg","34","34","34","39","47"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","780","780","780","790","670"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","740","740","740","780","670"]
["Kompresor","Type","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46"]
["","Gretje","Okolje","Min.","° CWB","-25","-25","-25","-25","-25"]
["","","","Maks.","° CWB","18","18","18","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","46","46","48","48","48"]
["","Gretje","","Visok","dBA","47","47","48","48","48"]
["Hladilno sredstvo","Tip","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Polnitev","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Polnjenje","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20","20","20","20","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","15","15","15","15","20"]
["Standardni pripomočki","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]