{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","30.6","30.6"]
["","","Ogrevanje","Izjemno nizka","m³/min","27.2","27.2"]
["","","","Izjemno nizka","cfm","1080","1080"]
["","","Ogrevanje","Izjemno nizka","cfm","960","960"]
["Mere","Enota","","Višina","mm","550","550"]
["","","","Širina","mm","858","858"]
["","","","Globina","mm","330","330"]
["Teža","Enota","","","kg","40","40"]
["Kompresor","Tip","","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","-10","-10"]
["","","","Maks.","° CDB","46","46"]
["","Gretje","Okolje","Min.","° CWB","-25","-25"]
["","","","Maks.","° CWB","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","48","48"]
["","","","Nizko","dBA","44","44"]
["","Gretje","","Visok","dBA","49","49"]
["","","","Nizko","dBA","45","45"]
["Hladilno sredstvo","Tip","","","","R-410A","R-410A"]
["","Polnitev","","","kg","1","1"]
["","Polnjenje","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","20","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - IU","Maks.","m","15","15"]
["Standardni pripomočki","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","220-240","220-240"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]