{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","49","","","52"]
["","","","Nizko","dBA","46","","","49"]
["","Hlajenje","","Nizko","dBA","46","","","49"]
["","","","Visok","dBA","49","","","52"]
["Standardni pripomočki","Izpustna obojka","","","","1","","","1"]
["","Priročnik za namestitev","","","","1","","","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Polnitev","","","kg","1.5","","","2.3"]
["","Tip","","","","R-410A","","","R-410A"]
["Cevni priklj.","Višinska razlika","IU - OU","Maks.","m","20","","","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","","","0,02 (za dolžino napeljave nad 10m)"]
["Sound power level","Hlajenje","","","dBA","","","","65"]
["Compressor","Type","","","","Hermetično zaprt nihajni kompresor","","","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Širina","mm","825","","","900"]
["","","","Globina","mm","300","","","320"]
["","","","Višina","mm","735","","","770"]
["Teža","Enota","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Frekvenca","","","Hz","50","","","50"]
["","Napetost","","","V","220-240","","","220-240"]
["Opombe","","","","","(1) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","(1) - 220V","","(1) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","(1) - 220V"]
["","","","","","(2) - Vsebuje fluorirane toplogredne pline","(2) - 230V","","(2) - Vsebuje fluorirane toplogredne pline","(2) - 230V"]
["Mere","Enota","","Višina","mm","","735","735","","770","770"]
["","","","Širina","mm","","825","825","","900","900"]
["","","","Globina","mm","","300","300","","320","320"]
["Teža","Enota","","","kg","","48","48","","71","71"]
["Compressor","Type","","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","","-10","-10","","-10","-10"]
["","","","Maks.","° CDB","","46","46","","46","46"]
["","Gretje","Okolje","Min.","° CWB","","-15","-15","","-15","-15"]
["","","","Maks.","° CWB","","18","20","","18","20"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","49","49","","52","52"]
["","","","Nizko","dBA","","46","46","","49","49"]
["","Gretje","","Visok","dBA","","49","49","","52","52"]
["","","","Nizko","dBA","","46","46","","49","49"]
["Hladilno sredstvo","Tip","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Polnitev","","","kg","","1.5","1.5","","2.3","2.3"]
["","Polnjenje","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","30","30","","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","","20","20","","20","20"]
["Standardni pripomočki","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Napajanje","Faza","","","","","1~","1~","","1~","1~"]
["","Frekvenca","","","Hz","","50","50","","50","50"]
["","Napetost","","","V","","220-240","220-240","","220-240","220-240"]
["Opombe","","","","","","(3) - 240V","","","(3) - 240V"]
["Standardni pripomočki","Drain socket","","","","","","1","","","1"]