{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","46.0"]
["","","Ogrevanje","Izjemno nizka","m³/min","46.0"]
["","","","Izjemno nizka","cfm","1624"]
["","","Ogrevanje","Izjemno nizka","cfm","1624"]
["Mere","Enota","","Višina","mm","770"]
["","","","Širina","mm","900"]
["","","","Globina","mm","320"]
["Teža","Enota","","","kg","71"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","730"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","730"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","-10"]
["","","","Maks.","° CDB","46"]
["","Gretje","Okolje","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","52"]
["","Gretje","","Visok","dBA","52"]
["Hladilno sredstvo","Tip","","","","R-410A"]
["","Polnitev","","","kg","2.3"]
["","Polnjenje","","","tCO2Eq","4.8"]
["","GWP","","","","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","20"]
["Standardni pripomočki","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Napajanje","Faza","","","","1~"]
["","Frekvenca","","","Hz","50"]
["","Napetost","","","V","220-240"]
["Opombe","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]