{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","47","","47","","48","48","48"]
["","Hlajenje","","Visok","dBA","46","","46","","48","48","48"]
["Standardni pripomočki","Spoj (odtok)","","","","1","","1"]
["","Priročnik za namestitev","","","","1","","1","","1","1","1"]
["Hladilno sredstvo","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Polnjenje","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Type","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Motor ventilatorja","Speed","Hlajenje","Izjwemno nizka","vrt/min","780","","780","","780","790","670"]
["","","Gretje","Izjwemno nizka","vrt/min","740","","740","","740","780","670"]
["Cevni priklj.","Višinska razlika","IU - OU","Maks.","m","15","","15","","15","15","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","0,02 (za dolžino napeljave nad 10m)","","0,02 (za dolžino napeljave nad 10m)","","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)","0,02 (za dolžino napeljave nad 10m)"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","","Hermetično zaprt nihajni kompresor","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Mere","Enota","","Width","mm","765","","765","","765","765","825"]
["","","","Globina","mm","285","","285","","285","285","300"]
["","","","Height","mm","550","","550","","550","550","735"]
["Teža","Unit","","","kg","34","","34","","34","39","47"]
["Ventilator","Hitrost pretoka zraka","Ogrevanje","Izjemno nizka","cfm","","","","","904","960","1,522"]
["","","Hlajenje","Izjemno nizka","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Phase","","","","1~","","1~","","1~","1~","1~"]
["","Frekvenca","","","Hz","50","","50","","50","50","50"]
["","Napetost","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","","(4) - SL: Tiha raven ventilatorja nastavitve hitrosti zračnega toka","","(4) - Vsebuje fluorirane toplogredne pline","(4) - Vsebuje fluorirane toplogredne pline","(4) - Vsebuje fluorirane toplogredne pline"]
["","","","","","(5) - Vsebuje fluorirane toplogredne pline","","(5) - Vsebuje fluorirane toplogredne pline"]
["Mere","Enota","","Višina","mm","","550","","550"]
["","","","Širina","mm","","765","","765"]
["","","","Globina","mm","","285","","285"]
["Teža","Enota","","","kg","","34","","34"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","","780","","780"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","","740","","740"]
["Kompresor","Tip","","","","","Hermetično zaprt nihajni kompresor","","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","° CDB","","-10","","-10"]
["","","","Maks.","° CDB","","46","","46"]
["","Gretje","Okolje","Min.","° CWB","","-15","","-15"]
["","","","Maks.","° CWB","","18","","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","46","","46"]
["","Gretje","","Visok","dBA","","47","","47"]
["Hladilno sredstvo","Tip","","","","","R-410A","","R-410A"]
["","Polnitev","","","kg","","1.0","","1.0"]
["","Polnjenje","","","tCO2Eq","","2.1","","2.1"]
["","GWP","","","","","2087.5","","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","20","","20"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","0,02 (za dolžino napeljave nad 10m)","","0,02 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","","15","","15"]
["Standardni pripomočki","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Napajanje","Faza","","","","","1~","","1~"]
["","Frekvenca","","","Hz","","50","","50"]
["","Napetost","","","V","","220-240","","220-240"]
["Standardni pripomočki","Izpustni čep","","","","","","","","1","1","1"]