{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Raven zvočnega tlaka","Gretje","","Visok","dBA","47","47","48","48"]
["","Hlajenje","","Visok","dBA","46","46","48","48"]
["Standardni pripomočki","Pokrovček izpusta","","","","1","1","","1"]
["","Priročnik za namestitev","","","","1","1","1","1"]
["","Oznaka polnitve hladilnega sredstva","","","","1","1","1"]
["","Večjezikovne oznake za fluorirane toplogredne pline","","","","1","1","Večjezikovne oznake za fluorirane toplogredne pline"]
["Hladilno sredstvo","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Polnjenje","","","kg","1.0","1.0","1.20","1.3"]
["","Tip","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","780","780","780","790"]
["","","Gretje","Izjwemno nizka","vrt/min","740","740","740","780"]
["Območje delovanja","Hlajenje","Okolje","Maks.","°CDB","46","46","46","46"]
["","","","Min.","°CDB","-10","-10","-10","-10"]
["","Ogrevanje","Okolje","Maks.","° CWB","18","18","18","18"]
["","","","Min.","° CWB","-15","-15","-15","-15"]
["Priključki cevne napeljave","Višinska razlika","IU - OU","Maks.","m","","","15"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","","0,020 (za dolžino napeljave nad 10m)"]
["Mere","Enota","","Širina","mm","765","765","765","765"]
["","","","Globina","mm","285","285","285","285"]
["","","","Višina","mm","550","550","550","550"]
["Kompresor","Tip","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Teža","Enota","","","kg","34","34","34","39"]
["Ventilator","Hitrost pretoka zraka","Gretje","Izjemno nizka","cfm","904","904","904","960"]
["","","","Izjemno nizka","m³/min","25.6","25.6","25.6","27.2"]
["","","Hlajenje","Izjemno nizka","m³/min","30.1","30.1","30.1","30.6"]
["","","","Izjemno nizka","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Faza","","","","1~","1~","1~","1~"]
["","Frekvenca","","","Hz","50","50","50","50"]
["","Napetost","","","V","220-240","220-240","220-240","220-240"]
["Opombe","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Vsebuje fluorirane toplogredne pline","(4) - Vsebuje fluorirane toplogredne pline","(4) - Vsebuje fluorirane toplogredne pline","(4) - Vsebuje fluorirane toplogredne pline"]
["Standardni pripomočki","Izpustni čep","","","","","","1"]
["Ventilator","Hitrost pretoka zraka","Hlajenje","Izjemno nizka","m³/min","","","","","48.9","45.0"]
["","","Ogrevanje","Izjemno nizka","m³/min","","","","","43.1","46.3"]
["","","","Izjemno nizka","cfm","","","","","1727","1589"]
["","","Ogrevanje","Izjemno nizka","cfm","","","","","1522","1635"]
["Mere","Enota","","Višina","mm","","","","","735","735"]
["","","","Širina","mm","","","","","825","825"]
["","","","Globina","mm","","","","","300","300"]
["Teža","Enota","","","kg","","","","","47","48"]
["Motor ventilatorja","Hitrost","Hlajenje","Izjwemno nizka","vrt/min","","","","","670"]
["","","Ogrevanje","Izjwemno nizka","vrt/min","","","","","670"]
["Kompresor","Tip","","","","","","","","Hermetično zaprt nihajni kompresor","Hermetično zaprt nihajni kompresor"]
["Območje delovanja","Hlajenje","Okolje","Min.","°CDB","","","","","-10","-10"]
["","","","Maks.","°CDB","","","","","46","46"]
["","Gretje","Okolje","Min.","° CWB","","","","","-15","-15"]
["","","","Maks.","° CWB","","","","","18","18"]
["Raven zvočnega tlaka","Hlajenje","","Visok","dBA","","","","","48","49"]
["","","","Nizko","dBA","","","","","44","46"]
["","Gretje","","Visok","dBA","","","","","48","49"]
["","","","Nizko","dBA","","","","","45","46"]
["Hladilno sredstvo","Tip","","","","","","","","R-410A","R-410A"]
["","Polnitev","","","kg","","","","","1.7","1.5"]
["","Polnjenje","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Priključki napeljave","Dolžina cevi","Maks.","OU - IU","m","","","","","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","","","","","0,020 (za dolžino napeljave nad 10m)","0,020 (za dolžino napeljave nad 10m)"]
["","Višinska razlika","IU - OU","Maks.","m","","","","","20.0","20"]
["Standardni pripomočki","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Napajanje","Faza","","","","","","","","1~","1~"]
["","Frekvenca","","","Hz","","","","","50","50"]
["","Napetost","","","V","","","","","220-230-240","220-230-240"]
["Opombe","","","","","","","","","","(1) - 230V"]