{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Mere","Enota","","Višina","mm","870","870"]
["","","","Širina","mm","1,100","1,100"]
["","","","Globina","mm","460","460"]
["Teža","Enota","","","kg","117","117"]
["Kompresor","Type","","","","Hermetično zaprt spiralni kompresor","Hermetično zaprt spiralni kompresor"]
["Operation range","Hlajenje","Okolje","Min.","° CDB","-20","-20"]
["","","","Maks.","° CDB","46","46"]
["","Gretje","Okolje","Min.","° CWB","-20","-20"]
["","","","Maks.","° CWB","15","15"]
["Sound power level","Hlajenje","","","dBA","73","76"]
["","Gretje","","","dBA","76 (1)","79 (1)"]
["Raven zvočnega tlaka","Hlajenje","","Nom.","dBA","53","57"]
["","Gretje","","Nom.","dBA","60","63"]
["Hladilno sredstvo","Tip","","","","R-32","R-32"]
["","Polnitev","","","kg","5","5"]
["","GWP","","","","675","675"]
["Priključki cevne napeljave","Tekočina","","Zun. premer","mm","9.52","9.52"]
["","Plin","","Zun. premer","mm","22.2","22.2"]
["","Dolžina napeljave","Maks.","OU - IU","m","100","100"]
["","","Sistem","Brez polnitve","m","30","30"]
["","Dodatno polnjenje hladilnega sredstva","","","kg/m","Glejte priročnik za namestitev","Glejte priročnik za namestitev"]
["Standardni pripomočki","Priročnik za namestitev","","","","1","1"]
["","Splošni varnostni previdnostni ukrepi","","","","1","1"]
["","Vezice","","","","2","2"]
["","Odlepite oznako za F-plin","","","","1","1"]
["","Priključne cevi","","","","6","6"]
["Power supply","Faza","","","","3~","3~"]
["","Frekvenca","","","Hz","50","50"]
["","Napetost","","","V","380-415","380-415"]
["Tok - 50 Hz","Maksimalni tok varovalk (MFA)","","","A","20","20"]
["Opombe","","","","","(1) - V skladu z ENER Lot 21","(1) - V skladu z ENER Lot 21"]